<        Installation instructions for Warp FixPak XR_W043















        

        
        



        October 18, 2000

        This FixPak makes the products it services Year 2000 ready
        
        Build level 8.267
        
        
        This FixPak applies to:
        
        XR_3005 Warp Server
        XR_3006 Warp Server SMP
        
        Requires Corrective Service Facility release f.143 or later
        
        OS/2 Fix Distribution
        Personal System Products
        Austin, Tx
        
        
        (c) Copyright International Business Machines Corporation, 1981, 1998.
        All rights Reserved.

        October 18, 2000 - Warp 3 FixPak XR_W043




                   October 18, 2000 - Warp 3 FixPak XR_W043

   CONTENTS


     1.0 Terms and Conditions  . . . . . . . . . . . . . . . . . . . . . . 1

     2.0 Do not use your system  . . . . . . . . . . . . . . . . . . . . . 2

     3.0 Installation Notes  . . . . . . . . . . . . . . . . . . . . . . . 3
       3.0.1 Out of memory or System error SYS0008 - Warp Server SMP   . . 3
       3.0.2 Device Drivers removed from Fixpak  . . . . . . . . . . . . . 3
       3.0.3 Please use Fixtool f.141 or later   . . . . . . . . . . . . . 3
       3.0.4 Can't install Warp 3  . . . . . . . . . . . . . . . . . . . . 3
       3.0.5 OS2DUMP split into two versions   . . . . . . . . . . . . . . 4
       3.0.6 Using Display Recovery Choices  . . . . . . . . . . . . . . . 5
       3.0.7 DSPINSTL.EXE failure  . . . . . . . . . . . . . . . . . . . . 5
       3.0.8 Additional diskette image for Warp v3 FixPaks   . . . . . . . 5
       3.0.9 Windows printer drivers leave a zombie thread running   . . . 6
       3.0.10 Updated Corrective Service Facility (CSF)  . . . . . . . . . 6
       3.0.11 Syslevel Correction Programs   . . . . . . . . . . . . . . . 7
       3.0.12 If Installing on a Preloaded System  . . . . . . . . . . . . 7
       3.0.13 Newer file on harddisk than is in FixPak   . . . . . . . . . 7
       3.0.14 CSF0208 No products were found   . . . . . . . . . . . . . . 8
       3.0.15 CSF0248 Archive path is shared between mismatched  . . . . . 8
       3.0.16 CSF0249 Error opening or creating archive file.    . . . . . 8
       3.0.17 Configuration Installation Distribution ( CID )  . . . . . . 8
       3.0.18 Read-Only files  . . . . . . . . . . . . . . . . . . . . . . 9
       3.0.19 DATABASE files removed from FixPak   . . . . . . . . . . . . 9

     4.0 Post Installation Notes  . . . . . . . . . . . . . . . . . . . . 10
       4.0.1 Setting IRQ9 processing in config.sys for VPIC.SYS   . . . . 10
       4.0.2 IPE on boot after FixPak 35 installed on UNI systems   . . . 10
       4.0.3 Installation of Java 1.1.4 or Java 1.1.6   . . . . . . . . . 11
       4.0.4 Files removed from FixPaks (33 and up)   . . . . . . . . . . 11
       4.0.5 DSPRES.DLL included in FixPaks   . . . . . . . . . . . . . . 11
       4.0.6 DOSCALL1.DLL Trap on Thinkpads that use MWAVE  . . . . . . . 11
       4.0.7 Trap D or E in LAN Distance  . . . . . . . . . . . . . . . . 12
       4.0.8 Screen corruption using Lotus Notes 4.1  . . . . . . . . . . 12
       4.0.9 Dell machines and font editing   . . . . . . . . . . . . . . 13

     5.0 New Function   . . . . . . . . . . . . . . . . . . . . . . . . . 14
     5.1 SES supported on SMP with FP38 or later  . . . . . . . . . . . . 14
     5.2 Querying file dates for files after Dec 31, 1999 in REXX   . . . 14
     5.3 Graphics Adapter Device Drivers (GRADD)  . . . . . . . . . . . . 15
     5.4 Serviceability (RAS) Enhancements  . . . . . . . . . . . . . . . 15
     5.5 Euro Support   . . . . . . . . . . . . . . . . . . . . . . . . . 16
       5.5.1 Base OS/2 support  . . . . . . . . . . . . . . . . . . . . . 16
       5.5.2 Where euro is not supported  . . . . . . . . . . . . . . . . 17
       5.5.3 Printing the euro  . . . . . . . . . . . . . . . . . . . . . 18
     5.6 New Print fuctions   . . . . . . . . . . . . . . . . . . . . . . 18
     5.7 IBM Open32   . . . . . . . . . . . . . . . . . . . . . . . . . . 18
     5.8 If you have installed OpenDoc  . . . . . . . . . . . . . . . . . 19

   
                                                                Contents  ii


                   October 18, 2000 - Warp 3 FixPak XR_W043

     5.9 Joliet-2 support in CDFS.IFS   . . . . . . . . . . . . . . . . . 19
     5.10 New (improved) CHKDSK   . . . . . . . . . . . . . . . . . . . . 20
       5.10.1 Using the new CHKDSK  . . . . . . . . . . . . . . . . . . . 20
       5.10.2 CHKDSK log formatter  . . . . . . . . . . . . . . . . . . . 22
     5.11 Automated Trap Screen Logging   . . . . . . . . . . . . . . . . 22
       5.11.1 SUPPRESSPOPUPS  . . . . . . . . . . . . . . . . . . . . . . 23
       5.11.2 TRAPLOG   . . . . . . . . . . . . . . . . . . . . . . . . . 23
     5.12 TRAPDUMP  . . . . . . . . . . . . . . . . . . . . . . . . . . . 23
     5.13 SYSDUMP   . . . . . . . . . . . . . . . . . . . . . . . . . . . 24
     5.14 Other README files  . . . . . . . . . . . . . . . . . . . . . . 24
     5.15 Reserve Drive Letters Added   . . . . . . . . . . . . . . . . . 25
     5.16 What is the SIQ (Single Input Queue) feature  . . . . . . . . . 26
       5.16.1 How it works  . . . . . . . . . . . . . . . . . . . . . . . 26
     5.17 Common File Dialog Interface changes  . . . . . . . . . . . . . 27

     6.0 Corrective Service Facility  . . . . . . . . . . . . . . . . . . 28
       6.0.1 Required CSF level   . . . . . . . . . . . . . . . . . . . . 28
       6.0.2 Where you can find CSF code  . . . . . . . . . . . . . . . . 28
       6.0.3 Creating FixPak diskettes  . . . . . . . . . . . . . . . . . 28

     7.0 Relocated OS/2 file support  . . . . . . . . . . . . . . . . . . 30

     8.0 LAN Server/Warp Server Remote IPL Considerations   . . . . . . . 31

     9.0 Installation Process   . . . . . . . . . . . . . . . . . . . . . 33
     9.1 Before installation  . . . . . . . . . . . . . . . . . . . . . . 33
     9.2 Method 1: Install from booted OS/2 partition.    . . . . . . . . 33
     9.3 Method 2: Boot from Corrective Service Disk 1.   . . . . . . . . 35
     9.4 Additional Corrective Service Facility information   . . . . . . 35

     10.0 CSD level of SYSLEVEL.OS2   . . . . . . . . . . . . . . . . . . 36
       10.0.1 New SYSLEVEL.FPK  . . . . . . . . . . . . . . . . . . . . . 37

     11.0 FixPak Corrective Service levels and disk layouts   . . . . . . 38

     12.0 Space Utilization   . . . . . . . . . . . . . . . . . . . . . . 58

     13.0 Recovering FixPak ARCHIVE and BACKUP space  . . . . . . . . . . 59

     14.0 Recovering from problems  . . . . . . . . . . . . . . . . . . . 60












   
                                                               Contents  iii


                   October 18, 2000 - Warp 3 FixPak XR_W043

   1.0 TERMS AND CONDITIONS

   Important - please read the following terms and conditions.

   Downloading the Service Fixes included in FixPak XR_W043 for OS/2 Warp 3
   indicates your acceptance of the following terms and conditions:

   1. You must be, and agree that you are, a current licensee of OS/2 Warp
      3.
   2. You may make copies of the OS/2 Service Fixes equal to the number of
      licensed copies of OS/2 Warp 3 you possess.
   3. You may only use the OS/2 Warp 3 Service Fixes included with FixPak
      XR_W043 for maintenance purposes.
   4. All other terms and conditions of your OS/2 Warp 3 license agreements
      apply to the Service Fixes; however, this does not extend any warranty
      and/or services, including but not limited to the "Initial
      Installation" period, outlined in such agreements.



































   
                                                     Terms and Conditions  1


                   October 18, 2000 - Warp 3 FixPak XR_W043

   2.0 DO NOT USE YOUR SYSTEM

   Once you begin a FixPak installation, do not try to use your system for
   any other purpose. Doing so may yield unexpected problems which can cause
   the FixPak installation to fail.















































   
                                                   Do not use your system  2


                   October 18, 2000 - Warp 3 FixPak XR_W043

   3.0 INSTALLATION NOTES



   3.0.1 OUT OF MEMORY OR SYSTEM ERROR SYS0008 - WARP SERVER SMP

   Customers who have had an "Out of memory" or SYS0008 problems on systems
   using Java should add the following line to the CONFIG.SYS file:

   Ž  SET JAVA_HIGH_MEMORY=1

   This will allow Java to move it't buffers to a lesser-used region of
   memory and may alleviate some memory constraints. There are no known
   unwanted side-effects to doing this.






   3.0.2 DEVICE DRIVERS REMOVED FROM FIXPAK

   Beginning with Warp 4 FixPak XR_M011 and Warp 3 FixPak XR_W041, most OS/2
   Device Drivers have been moved to a separate Device Driver FixPak. The
   first Device Driver FixPak, XR_D001, is now available where this FixPak
   is available.

   To avoid potential Device Driver problems with the installation of Warp 4
   FixPak XR_M011 and Warp 3 FixPak XR_W041, your system should be at FixPak
   level XR_M005 or higher for Warp 4 and XR_W032 or higher for Warp 3.


   3.0.3 PLEASE USE FIXTOOL F.141 OR LATER

   Beginning with Warp 3 FixPak 40 and Warp 4 FixPak 10, you must use
   Corrective Service Facility f.141 or later.  It has fixes for problems
   found in the F.138B and F.139 builds as well as a fix to support RIPL
   servers where there may be in excess of 250 SYSLEVEL files. It also
   handles the type 1 (All FixPaks prior to 40 and 10) and type 2 (FixPaks
   40 and 10 and later) FixPaks.

   If you try to use a CSF level prior to F.138B you will get a "CSF0208 No
   products were found on the target system to service" message.


   3.0.4 CAN'T INSTALL WARP 3

   If you can't get Warp 3 installed, check the OS/2 Device Driver Pak
   Online at:



   
                                                       Installation Notes  3


                   October 18, 2000 - Warp 3 FixPak XR_W043

   http://service.software.ibm.com/os2ddpak/readme.htm#disk1


   for the latest available device drivers to update your Installation disks
   with.


   3.0.5 OS2DUMP SPLIT INTO TWO VERSIONS

   OS2Dump has been split into two versions. If you are installing this
   fixpak on PS/2 model 9595 machines, use the version located on the last
   fixpak diskette.  Also, if you are running older hardware (486s or early
   Pentiums), you may wish to use the OS2Dump located on the last fixpak
   diskette.

   We have encountered some problems with early implementations of the PCI
   Bus BIOS extensions (INT 1A) on certain processors and BIOS levels. We
   are not sure how many different machines and BIOSes are affected. We do
   know many of the PS/2 model 9595s have the problem. The end result of
   this is that the version of OS2Dump which supports PCI Bus machines does
   not work on some older hardware.  In order to continue to support the
   full range of hardware that OS/2 runs on, we have divided OS2Dump into a
   PCI version and an non-PCI version. If you are running fairly recent
   hardware, the PCI version of OS2Dump will work on your machine whether or
   not it has a PCI bus. All BIOS problems have been worked out.

   To reiterate, the problem occurs only on older hardware. If you are
   running a 486 or early Pentium (P60 or less), you may wish to use the
   non-PCI version located on the last fixpak diskette. If you are running a
   9595, you must use the non-PCI version located on the last fixpak
   diskette.

    If, after installing this FixPak, you encounter problems taking a
   standalone dump and your system fits description above, perform the
   following steps to install the non-PCI version of OS2DUMP located on last
   disk of this FixPak:

   1. Open an OS/2 window.
   2. Change to drive letter where OS/2 is installed.
   3. Enter "cd\" to get to the root directory.
   4. Enter OS/2 command "attrib -s -h -r os2dump" to unhide OS2DUMP.
   5. Enter "ren os2dump os2dump.pci"; save PCI version of OS2DUMP.
   6. Insert last disk of FixPak in drive A.
   7. Copy a:\os2dump
   8. Enter OS/2 command "attrib +r +s +h os2dump" to hide OS2DUMP.
   9. Reboot system.






   
                                                       Installation Notes  4


                   October 18, 2000 - Warp 3 FixPak XR_W043

   3.0.6 USING DISPLAY RECOVERY CHOICES

   If you have the "Display Recovery Choices at each system startup"
   function active on your system, you need to disable it before you apply a
   FixPak if

   Ž  The system is running
   Ž  The boot partition will be serviced.

   The problem with using this function is that the Corrective Service
   Facility (CSF) updates the current CONFIG.SYS with entries to run the
   Locked File Device Driver (LFDD) the next time you boot the system. This
   is done to replace files that are currently in use (locked) by the
   system.

   The Recovery choices function replaces the current CONFIG.SYS with the
   one that is associated with the recovery choice you select, wiping out
   the LFDD entries. This means the LFDD does not run at boot time and the
   deferred files will not get updated, therefore the FixPak does not get
   completely applied.

   Note: It is not necessary to disable this function if you install a
   FixPak by booting from the CSF disks or from another OS/2 partition.


   3.0.7 DSPINSTL.EXE FAILURE

   DSPINSTL.EXE may fail when installing OEM versions of non-IBM video
   device drivers. For Uni-processor versions of Warp, the archived version
   of the file can be used as a workaround. For SMP versions, contact IBM
   for a temporary fix.  A subsequent FixPak will correct this problem.


   3.0.8 ADDITIONAL DISKETTE IMAGE FOR WARP V3 FIXPAKS

   We've added an additional diskette image to Warp v3 FixPaks. This disk
   contains the directories and tools previously found on the last FixPak
   disk.

   This disk may contain the following:

   Ž  BETA
   Ž  DIR_ONE
   Ž  DIR_TWO
   Ž  SYSLEVEL
   Ž  FIXSYSL.CMD         (US only)
   Ž  SYSZMPM.CMD         (non-US only)
   Ž  UPDTRIPL.EXE

   Note: This DOES NOT increase the size of the FixPak


   
                                                       Installation Notes  5


                   October 18, 2000 - Warp 3 FixPak XR_W043

   The SYSLEVEL directory contains corrected SYSLEVEL files for National
   Language Versions (NLV) of Warp v3 products. The directory names have the
   following meanings:

   Ž  Directory Product
   Ž  --------- -------------------------------------------------------
   Ž  WARPSRV   XR_3005 Warp Server
   Ž  WRPSVSMP  XR_3006 Warp Server SMP



   3.0.9 WINDOWS PRINTER DRIVERS LEAVE A ZOMBIE THREAD RUNNING

   A problem occurs with some Windows printer drivers where a zombie thread
   is left running  after the program that loaded it is exited.

   This does not occur when the program is run from a Seamless instance of
   PROGMAN or from a Full Screen session because when these are exited the
   whole WINOS2 Subsystem is exited.

   This problem has been reported for the Adobe and Hewlett Packard Windows
   printer drivers. To correct this problem for people running with these
   drivers ONLY who have experienced symptoms such as:

   Ž  exiting a program running seamlessly after printing or
   Ž  setting up a printer and seeing the icon not being unhatched and/or
   Ž  not being able to start another copy of the program

   Add the following line in OS2\MDOS\WINOS2\SYSTEM.INI in the *boot*
   section:

   Ž  backgroundtasks=run_enum.exe,hpfbkg02.exe

   then restart WINOS2.

   Note: There may be other drivers that have the same problem.  If you
   experiences a similar problem with other drivers, please report it so the
   correct SYSTEM.INI entry can be determined.



   3.0.10 UPDATED CORRECTIVE SERVICE FACILITY (CSF)

   Use CSF level f.141 or later for all Fixpaks.  It is contained in
   CS_140.EXE.  This is a self-extracting ZIP file.  It is not and does not
   contain bootable disks.

   See the READ.ME file for instructions on how to boot with diskettes along
   with a lot of other useful information.



   
                                                       Installation Notes  6


                   October 18, 2000 - Warp 3 FixPak XR_W043

   3.0.11 SYSLEVEL CORRECTION PROGRAMS

   The FIXSYSL.CMD, located on the last disk of US FixPaks, is included for:

   1. Warp systems that have applied an S3 video pak and the Current CSD
      level is XR02110 (execute the syslevel command to find out);

   2. APTIVA systems with a Current CSD level XR03005, Compid 562260100,
      Type WP.

   This program will set the Current CSD level to XR03002.  Please run the
   FIXSYSL program before installing this FixPak.

   The SYSZMPM.CMD, located on the last disk of non-US FixPaks, is included
   for:

   1. Warp Server SMP systems that have a Current CSD Level of XR06200 and a
      Prior CSD Level of UN09407 in the \MMOS2\INSTALL\SYSLEVEL.MPM file.

   2. Other Warp systems with incorrect Multimedia syslevel files.

   This program will set the Current CSD level to XR03006 to allow service
   to be applied to Multimedia files.  Please run the SYSZMPM program before
   installing this FixPak on Warp Server SMP systems.


   3.0.12 IF INSTALLING ON A PRELOADED SYSTEM

   Installing this FixPak on systems that were preloaded may cause a pop-up
   to occur that is invalid.  The pop-up claims that the following files
   have a more recent date and/or version than the ones contained on your
   system:

       MMOS2\DLL\IOPRNLS.DLL
       MMOS2\DLL\AMPMXMCD.DLL
       MMOS2\DLL\AUDIOMCD.DLL
       MMOS2\DLL\AUDIOSH.DLL
       MMOS2\DLL\MMPM.DLL
       OS2\INSTALL\SYSLEVEL.SUC


   The proper action is to allow the FixPak installation to overwrite these
   files with the ones supplied by the FixPak.


   3.0.13 NEWER FILE ON HARDDISK THAN IS IN FIXPAK

   If you get a popup stating that a newer file exists on your harddisk than
   is in the FixPak. press the "OK" button unless you know for sure the file
   on your harddisk is newer than the one in the Fixpak.


   
                                                       Installation Notes  7


                   October 18, 2000 - Warp 3 FixPak XR_W043

   3.0.14 CSF0208 NO PRODUCTS WERE FOUND

   This means no SYSLEVEL files was found that had a CSD Level, COMPID,
   Version and Type that matched any of the SYSLEVEL files supported by this
   FixPak. Run the SYSLEVEL command and record the output for SYSLEVEL.OS2
   in the OS2/INSTALL directory on your boot drive. Compare this data with
   the data contained in the README.1ST file on FixPak disk 1.

   To recover from this, rename the existing SYSLEVEL.OS2 file to SYSL.OS2
   and copy SYSLEVEL.OS2 from your Warp 4 installation DISK 1.


   3.0.15 CSF0248 ARCHIVE PATH IS SHARED BETWEEN MISMATCHED

   1. The Archive path you specified (or was previously specified) contains
      files from a different release of OS/2. You need to specify a
      different Archive path.
   2. You have a bad SYSLEVEL.OS2 or SYSLEVEL.MPM file. Both must have the
      same Current CSD Level, Version, Type and Component ID if you point
      both FixPak Archives to the same location.

      Check \OS2\INSTALL\SYSLEVEL.OS2 and \MMOS2\INSTALL\SYSLEVEL.MPM. If
      either is wrong, place the last FixPak disk in A: and run FIXSYSL.CMD
      to correct SYSLEVEL.OS2 problems or SYSZMPM.CMD to fix SYSLEVEL.MPM
      problems.



   3.0.16 CSF0249 ERROR OPENING OR CREATING ARCHIVE FILE.

   Typically this means the FixPak Archive directory has been deleted but
   the files that point to it still exist. You need to delete the
   LOGF000.OS2 and LOGSTART.OS2 files from your OS2/INSTALL directory.
   LOGSTART.OS2 has the R/O attribute set and it needs to be reset before
   the file can be deleted.  There may also be a LOGARCH.OS2 file that needs
   to be deleted.

   This can also occur for Multi Media Presentation Manager/2 (MMPM). You
   would then need to delete the LOGF0000.MPM and LOGSTART.MPM files from
   the \MMOS2\INSTALL directory and possibly LOGARCH.MPM if it exists.


   3.0.17 CONFIGURATION INSTALLATION DISTRIBUTION ( CID )

   Read the README.CID on Disk # 1 for an example of how to set up a
   response file to do a CID install.






   
                                                       Installation Notes  8


                   October 18, 2000 - Warp 3 FixPak XR_W043

   3.0.18 READ-ONLY FILES

   If you installed OS/2 Warp 3.0 from a CD-ROM, some files being updated
   may have the Read-Only attribute set. This will cause the update program
   to ask you if you want the files replaced. Answer OK.


   3.0.19 DATABASE FILES REMOVED FROM FIXPAK

   DATABASE.TXT and DATABASE.DAT files have been removed from FixPak 29 and
   will be left out of all future FixPaks.  They are used to control the
   Notebook settings for migrated applications during initial install or
   selective install.

   This has been done to protect customers who have customized these files.





































   
                                                       Installation Notes  9


                   October 18, 2000 - Warp 3 FixPak XR_W043

   4.0 POST INSTALLATION NOTES



   4.0.1 SETTING IRQ9 PROCESSING IN CONFIG.SYS FOR VPIC.SYS

   Some applications like PCAS (and some terminal emulators) have problems
   sharing IRQ9 in a VDM.  Since the DOS Virtual Device drivers are not
   loaded out of CONFIG.SYS, a new device driver VPICPARM.SYS has been added
   starting with Warp 3 FixPak 38 and Warp 4 FixPak 8.

   To prevent sharing of IRQ9 in a VDM, add the following statement in
   config.sys:

      device=x:\os2\mdos\vpicparm.sys irq9_off
      (x: is your OS/2 boot drive)


   Next, in the settings for the program that requires exclusive access to
   IRQ9, set the DOS setting HW_SHARE_IRQ9 to ON.

   When you next boot your system, VDMs will not share IRQ9.


   4.0.2 IPE ON BOOT AFTER FIXPAK 35 INSTALLED ON UNI SYSTEMS

   If you experience a kernel trap (black screen trap) or get a messages
   stating that device drivers (such as CLOCK01.SYS) were not able to
   install at boot time do the following:

   1. Reboot and press Alt-F1 when the white block appears
   2. Select C for command line
   3. From the command line enter: TEDIT CONFIG.SYS
   4. Add the following statement to the end of CONFIG.SYS:

      TRACE=OFF,6


   5. Reboot

   Note: DO NOT use major code 6 trace events either from CONFIG.SYS or from
   the command line.

   A fix for this problem will be placed on "ftp://service.boulder.ibm.com"
   in the "ps/products/os2/fixes/v3.0warp/english-us/xr_w035/" directory and
   the NCS Support News page at
   "http://ps.boulder.ibm.com/pbin-usa-ps/getobj.pl?/pdocs-usa/fixnews.html"
   will be updated when the fix is available.




   
                                                 Post Installation Notes  10


                   October 18, 2000 - Warp 3 FixPak XR_W043

   4.0.3 INSTALLATION OF JAVA 1.1.4 OR JAVA 1.1.6

   Installation of Java 1.1.4 or Java 1.1.6 on top of this FixPak will
   down-level portions of the ULS support if you are not using the 1.2.2 (or
   later) level of Feature Installer.

   If this occurs, Euro currency support will not work correctly. To
   recover, re-install this FixPak. This will allow both Java and Euro
   support to work correctly.


   4.0.4 FILES REMOVED FROM FIXPAKS (33 AND UP)

   The following files, introduced in FixPak 26, have been merged into
   LOCALE.DLL and were removed from FixPak 33 and all future Warp 3 FixPaks.

      AR_AA.DLL  EN_CA.DLL  FR_CA.DLL  LT_LT.DLL  SH_BA.DLL
      BG_BG.DLL  EN_GB.DLL  FR_CH.DLL  LV_LV.DLL  SK_SK.DLL
      C.DLL      EN_IE.DLL  FR_FR.DLL  MK_MK.DLL  SL_SI.DLL
      CA_ES.DLL  EN_NZ.DLL  HR_HR.DLL  NL_BE.DLL  SQ_AL.DLL
      CS_CZ.DLL  EN_US.DLL  HU_HU.DLL  NL_NL.DLL  SR_SP.DLL
      DA_DK.DLL  EN_ZA.DLL  IS_IS.DLL  NO_NO.DLL  SV_SE.DLL
      DE_AT.DLL  ES_ES.DLL  IT_CH.DLL  PL_PL.DLL  TH_TH.DLL
      DE_CH.DLL  ES_LA.DLL  IT_IT.DLL  PT_BR.DLL  TR_TR.DLL
      DE_DE.DLL  ET_EE.DLL  IW_IL.DLL  PT_PT.DLL  UNIV.DLL
      EL_GR.DLL  FI_FI.DLL  JA_JP.DLL  RO_RO.DLL  ZH_CN.DLL
      EN_AU.DLL  FR_BE.DLL  KO_KR.DLL  RU_RU.DLL  ZH_TW.DLL


   Additionally, ENULS.MSG was removed from FixPak 33 (and up) as it is no
   longer needed.


   4.0.5 DSPRES.DLL INCLUDED IN FIXPAKS

   DSPRES.DLL has been added to FixPak 35 and up for support of Euro
   character display. This file can sometimes be overwritten by video device
   driver installation. If this occurs, an updated version is located in
   \OS2\INSTALL\VGA. This updated file can be copied into the \OS2\DLL
   directory.


   4.0.6 DOSCALL1.DLL TRAP ON THINKPADS THAT USE MWAVE

   After installing this FixPak on a Thinkpad that uses MWAVE and the LAN
   while in a docking station you may encounter a DOSCALL1.DLL trap after
   rebooting when the machine is undocked.

   A fix has been made to the MWAVE MWNOTOS2.EXE to correct this problem.
   The MWNOTOS2.EXE file can be found on the Internet along with a readme
   (.doc file) on how to replace the file. The location is:

   
                                                 Post Installation Notes  11


                   October 18, 2000 - Warp 3 FixPak XR_W043

   Point your Web browser at:

   ftp://www3.pc.ibm.com/pub/pccbbs/mobiles/mwnotos2.exe
   ftp://www3.pc.ibm.com/pub/pccbbs/mobiles/mwnotos2.doc




   4.0.7 TRAP D OR E IN LAN DISTANCE

   If you get a Trap D or E in the MACFH$1 device driver, at offset 126C,
   while running LAN Distance, please call IBM Service for the LAN Distance
   APAR IC14228.


   4.0.8 SCREEN CORRUPTION USING LOTUS NOTES 4.1

   There is a screen corruption problem when running Lotus Notes 4.1 in 256
   colors on OS/2.  This problem has been corrected in version 4.1.2.
   Symptoms normally appear as anomilies in the fonts, such as parts of
   characters or entire characters disappearing.  This corruption can occur
   at any resolution.

   Since this only occurs when using 256 colors, an immediate work around is
   to not use 256 colors.  To change the number of colors displayed:

   1. open the OS/2 System folder

   2. open the System Setup folder

   3. double click on the System icon in the System Setup folder

   4. select a resolution that does not use 256 colors

   5. close the folders

   6. shutdown and reboot the machine

   The fix for this problem is in the display device drivers. IBM supported
   display device drivers will be available on the PCCBBS and Internet as
   "Controlled" fixes. You should contact the IBM PSP Software Solution
   Center at 1-800-992-4777 to obtain PCCBBS and Internet logon information
   for display device drivers needed. The build level should be 0.041 or
   above.

   See "Where Fixes can be found" for where display device drivers can be
   found once they have been publically released.





   
                                                 Post Installation Notes  12


                   October 18, 2000 - Warp 3 FixPak XR_W043

   4.0.9 DELL MACHINES AND FONT EDITING

   When editing fonts, users of Dell machines may discover a slight
   regression.  When a font size is edited, the Font Palette is updated
   correctly; however, should users browse (select around) the palette, they
   might, at times, notice an inconsistency between the font size displayed
   on the palette and the one that is displayed on the font editor.  In all
   cases, the font size displayed on the Font Palette is the correct size
   for the font when it is dragged to the target (for example, the desktop,
   folder, or application).










































   
                                                 Post Installation Notes  13


                   October 18, 2000 - Warp 3 FixPak XR_W043

   5.0 NEW FUNCTION

   It is our policy not to include new function in FixPaks. However, as with
   any policy there may be exceptions. If any exception occurs in the
   future, we will communicate them to you in this section of the
   README.1ST.

   We apologize for not communicatiing this more clearly earlier and
   specifically for not including information on IBM Open32 in the FixPak 26
   (and subsequent) README.1ST.


   5.1 SES SUPPORTED ON SMP WITH FP38 OR LATER

   SES is supported on systems running Warp Server SMP once FixPak 38 or
   later is installed.

   You can get the IBM OS/2 Security Enabling Services from the Web at:

   ftp://service.boulder.ibm.com/ps/products/os2/warp.update.kit/warpses/




   5.2 QUERYING FILE DATES FOR FILES AFTER DEC 31, 1999 IN REXX

   Existing REXX functions return file dates with a two digit year only.
   While these functions are Year 2000 tolerant (i.e. the results will be
   correct for files dated after Dec 31, 1999) they require some additional
   logic in existing programs to handle the returned date correctly when
   they are compared with other file dates.

   Since the output format of the exisiting functions could not be changed
   for compatibility reasons, new options have been added to the REXX
   interpreter to return file dates with the year formatted with 4 digits.
   Two functions have been extended to support the new format. The syntax to
   retrieve the file date in 4 digit format is as follows:















   
                                                            New Function  14


                   October 18, 2000 - Warp 3 FixPak XR_W043

      /********************************************/
      /* Use STREAM QUERY TIMESTAMP to query file */
      /* date in 4 digit format                   */
      /********************************************/
      Say Stream("C:\CONFIG.SYS", "C", "QUERY TIMESTAMP")

      /***********************************************/
      /* Use option "L" with SysFileTree to return a */
      /* list of files with long date format         */
      /***********************************************/
      Call RxFuncAdd "SysLoadFuncs", "RexxUtil", "SysLoadFuncs"
      Call SysLoadFuncs
      Call SysFileTree "C:\*.*", "Files", "L"
      Do i = 1 To Files.0
         Say Files.i
      End


   These extensions are available in both classic REXX and Object REXX on
   OS/2 Warp 3 and Warp 4 since fix pack versions 35 and 6. If you use these
   extensions in your program you have to make sure that you are running the
   right level of REXX


   5.3 GRAPHICS ADAPTER DEVICE DRIVERS (GRADD)

   GRADD is supported on all Warp 3 releases beginning with FixPak 35.

   Future updates for GRADD and other video drivers (when they are released)
   will be found via the internet at:

   Ž  http://service.software.ibm.com/pslaunch.html



   5.4 SERVICEABILITY (RAS) ENHANCEMENTS

   With FixPak 35 for Warp 3.0 and FixPak 10 for Warp 4.0 major enhancements
   were provided to the system diagnostic tools (RAS Enhancements).  They
   provide major functional enhancements to the System Trace and Process
   Dump facilities.  Full details of these enhancements can be found in the
   README.DBG file that will be found in the \OS2\INSTALL directory after
   this FixPak is installed.

   Other associated documentation may be found in:

   Ž  OS2\SYSTEM\RAS\TRACE.DOC
   Ž  OS2\SYSTEM\RAS\DTRACE.DOC
   Ž  OS2\SYSTEM\RAS\PROCDUMP.DOC
   Ž  OS2\SYSTEM\RAS\TRSPOOL.DOC


   
                                                            New Function  15


                   October 18, 2000 - Warp 3 FixPak XR_W043

   Always refer to README.DBG for details of any RAS enhancements delivered
   with a FixPak.


   5.5 EURO SUPPORT

   The European Monetary Union is creating the euro as a new common currency
   for Europe.  As part of this effort the European Commission has
   introduced a new character which represents the euro.  This character
   looks like an uppercase C with two horizontal lines through it.  The euro
   will come into existence on January 1, 1999 for use in banking.  Euro
   notes and coins will be issued starting January 2002.



   5.5.1 BASE OS/2 SUPPORT

   The OS/2 basic support for Euro consists of adding the euro character to
   fonts, codepages, and keyboards.  The euro is added to all display and
   ATM fonts and to the Times New Roman MT 30 TrueType font which is
   available with Java 1.1.  The euro is added to all western European
   keyboards and the US International keyboard.  The euro can be used in
   base OS/2, Presentation Manager, and in DOS.  The euro is not supported
   in WinOS2.

   The euro character is added to these OS/2 base and PM codepages:

       850    0xD5   PC Latin 1          base + PM
       857    0xD5   PC Turkish          base + PM
       1004   0x80   Windows Extended    base + PM
       1250   0x80   Windows Latin 2     PM
       1251   0x88   Windows Cyrillic    PM
       1252   0x80   Windows Latin 1     PM
       1254   0x80   Windows Turkish     PM
       1257   0x80   Windows Baltic      PM


   The euro character is added to these fonts.

       Courier                      (bitmap)
       Courier                      (ATM)
       Helv                         (bitmap)
       Helvetica                    (ATM)
       System Monospace             (bitmap)
       System Proportional          (bitmap)
       System VIO                   (bitmap)
       Times New Roman              (ATM)
       Times New Roman MT 30        (TrueType - Java 1.1)
       Tms Rmn                      (bitmap)
       WarpSans                     (bitmap)


   
                                                            New Function  16


                   October 18, 2000 - Warp 3 FixPak XR_W043

   The euro character is added to these OS/2 keyboards:

       Belgium           be       altgr-e
       Canada            ca       altgr-e
       Canadian French   cf       altgr-e
       Denmark           dk       altgr-5
       Finland           su (fi)  altgr-5
       France            fr       altgr-e
       Germany           gr (de)  altgr-e
       Germany(453)      de453    altgr-e
       Iceland           ic (is)  altgr-5
       Iceland 101       is458    altgr-5
       Italy             it       altgr-5
       Italy extended    it142    altgr-5
       Latin America     la       altgr-e
       Netherlands       nl       altgr-e
       Norway            no       altgr-5
       Portugal          po       altgr-5
       Spain             sp (es)  altgr-5
       Sweden            sv       altgr-5
       Swiss French      sf       altgr-e
       Swiss German      sg (sd)  altgr-e
       Turkey            tr179    altgr-e
       Turkey 440        tr440    altgr-e
       UK                uk       altgr-4
       UK 168            uk168    altgr-e
       US International  ux       altgr-e





   5.5.2 WHERE EURO IS NOT SUPPORTED

   The euro is not supported in WinOS2.  This character is not supported in
   the Windows-1252 codepage used in WinOS2.  This character is not
   available on the WinOS2 keyboards.  This character is not available in
   the WinOS2 supplied TrueType fonts:

           Arial             (Windows TrueType)
           Courier New       (Windows TrueType)


   The euro is not in the 437 (US English) or 863 (Canadian French)
   codepages.  You must use codepage 850 to get the euro.  The euro is not
   on the US keyboard.  You can use the US International (ux) keyboard
   instead.





   
                                                            New Function  17


                   October 18, 2000 - Warp 3 FixPak XR_W043

   5.5.3 PRINTING THE EURO

   Existing printers do not support the euro in device fonts.  You need to
   select a font which is not mapped to a device font in order to print the
   euro.  The euro will print correctly on printers where the system fonts
   are used.  When there are problems, a dotless-i is normally printed
   instead of the euro.

   For PostScript printers, it is necessary to disable device fonts to print
   the euro in one of the base PostScript fonts (Helvetica, Times Roman,
   Courier).  To do this:

   1. Open the properties of the Printer object
   2. Select the Print Driver tab
   3. Select Job Properties
   4. Select the Output tab
   5. Deselect "Use printer device fonts"




   5.6 NEW PRINT FUCTIONS

   The following print functions have been added starting at FixPak XR_W031
   level:

   Ž  Allow moving a print job from one print server to another server.
   Ž  Allow moving all print jobs at once.
   Ž  Define a backup print queue so that when a printer has problems, all
      jobs will be sent to a backup print queue if the problem persists for
      a specified number of minutes.
   Ž  When creating a network print object, user will be prompted to create
      a WINOS2 print configuration.



   5.7 IBM OPEN32

   Open32 is a new API set provided in OS/2 Warp 3 beginning with FixPak 26
   to help ISVs migrate their Windows 32-bit applications to OS/2.
   Approximately 750 APIs from the Win32 API set are included and provide
   essentially the same functionality as the Windows NT 3.51 APIs of the
   same name.

   Applications such as Lotus SmartSuite 96 are enable by this set of APIs.

   It is required that Open32 support be installed on OS/2 Warp 3 systems
   that have FixPak 26 or higher installed. The Open32 code requires 20MB of
   disk space on your OS/2 Warp 3 boot drive.



   
                                                            New Function  18


                   October 18, 2000 - Warp 3 FixPak XR_W043

   It also creates a new \LANGUAGE directory on your boot drive and adds SET
   ULSPATH=x:\LANGUAGE to CONFIG.SYS (x: is your boot drive).

   If you are installing this FixPak on a machine that has an older version
   of IBM Open32 (formerly known as Developer API Extensions or DAX) from
   either FixPak 17 Special Edition or DevCon 9, then you must uninstall the
   older version of Open32 before starting to install this new version.

   If you no longer have the CD or diskettes to uninstall the older version
   of Open32 then you must follow these steps:

   1. In config.sys, delete the following line:

         RUN=x:\OS2\RSRV.EXE
       where x: is your boot drive.


   2. Reboot your system
   3. Delete the following files from your machine, where x: is your boot
      drive.

         x:\boot.dat
         x:\registry.dat
         x:\dos.dat
         x:\os2\rsrv.exe
         x:\os2\install\inst_dos.exe
         x:\os2\install\reginit exe




   5.8 IF YOU HAVE INSTALLED OPENDOC

   If you have installed OpenDoc parts for Multimedia and you wish to keep
   your OpenDOc support then DO NOT update Multimedia at all. To do this,
   use the A:\SERVICE installation method and do not select Multimedia as a
   product to be serviced.


   5.9 JOLIET-2 SUPPORT IN CDFS.IFS

   Joliet is a Microsoft extension to the ISO 9660 CD-ROM file system which
   adds Unicode and longname support.  Presently both Windows 95 and Windows
   NT 4.0 support the Joliet-2 and Joilet-3 formats.  Beginning with Warp 3
   Fixpak 32 and Warp 4 Fixpak 4, you can enable the Joliet-2 support by
   adding the '/w' option to the CDFS.IFS statement in CONFIG.SYS.

   Joilet-3 format is not supported.




   
                                                            New Function  19


                   October 18, 2000 - Warp 3 FixPak XR_W043

   5.10 NEW (IMPROVED) CHKDSK

   This new version of CHKDSK offers significant improvements for High
   Performance File System (HPFS) drives.  CHKDSK now fixes all errors found
   on HPFS drives in a single pass, operating faster, and with less memory
   than previous versions.  It contains better error detection and
   correction algorithms, and creates a log file so service personnel can
   determine what errors it found and how it corrected them.  Finally, only
   the amount of physical memory in your system limits the size of the
   largest drive CHKDSK can check at boot time (autocheck).

   Improvements in this version of CHKDSK are for HPFS drives only.  No
   changes occurred to checking File Allocation Table (FAT) drives.  This
   enhanced CHKDSK operates on IBM OS/2 Warp 3.0 and higher, including IBM
   Warp 4, IBM Warp Server 4 and IBM Warp Server 4 SMP.  This new CHKDSK
   version will not run on version of OS/2 before OS/2 Warp 3.0.


   5.10.1 USING THE NEW CHKDSK

   The interface to CHKDSK remains CHKDSK.COM and PMCHKDSK.  No changes
   occurred to the CHKDSK command line parameters or messages.

   The first time this version of CHKDSK runs on a fast formatted drive, it
   will report harmless errors.  These errors go away once CHKDSK is run
   with the /F option.

   Note: OS/2 Warp Install uses fast format.

   Unlike prior versions of CHKDSK, large drives ( > 8GB) may be autochecked
   if sufficient memory is available.  The amount of memory required can
   vary between 16MB and 48MB depending on the size of the drive.  To enable
   the autochecking of large drives, the following line must be added to
   your config.sys:

     BASEDEV=CHKDSK.SYS


   This device driver allows CHKDSK to access memory normally reserved for
   the system during the boot process.  Due to this, if CHKDSK has to use
   this memory:

   Ž  The memory will not be available for the system to use in completing
      the boot process
   Ž  Errors may occur later in the boot process.

   Hence, the chkdsk.sys device driver is smart enough to recognize when
   CHKDSK has used this reserved memory and will reboot the system
   automatically after all HPFS drives have been checked.  Since the drives
   were checked before the reboot, CHKDSK will not have to check them after
   the reboot and the system will boot normally.

   
                                                            New Function  20


                   October 18, 2000 - Warp 3 FixPak XR_W043

   Note: For those wishing to run unattended:  In order to prevent the
   system from pausing between autocheck and the reboot, we recommend that
   the statement PAUSEONERROR=NO be in the CONFIG.SYS.

   When you don't have enough physical (real) memory to autocheck large
   drives, you must use virtual memory from SWAPPER.DAT.  The technique is
   to check the large drives between the time OS/2 starts and PM begins.  To
   start OS/2, the swap file and device drivers must reside on an unaffected
   drive.  The drives to be checked must not appear in the autocheck list in
   the IFS statement for HPFS (or HPFS386).

   This technique involves the following steps:

   1. Remove the drive letter of the affected drive(s) from the autocheck
      list in the IFS statement for HPFS (or HPFS386).
   2. If you are using HPFS, add /QUIET to the IFS statement for HPFS.
   3. If you are using HPFS386.IFS, add POPUPERRORS=NO below the
      [filesystem] section of the HPFS386.INI file. Support for the
      POPUPERRORS parameter requires OS/2 LAN Server FixPak IP08265 or
      higher for LS 5.0 or FixPak IP08503 or higher for LS 5.1. In addition,
      the POPUPERRORS parameter ONLY suppresses HFS0102 messages.
   4. Add a CALL statement to your config.sys.  This CALL statement will
      call CHKDSK.COM, and will tell it what drive to check. This CALL
      statement must appear after the LIBPATH=, SET PATH=, and SET DPATH=
      statements, but before any other CALL statements in your CONFIG.SYS
      file.

   Calls to CHKDSK in STARTUP.CMD are not necessary, when using this method
   or the base device driver (chkdsk.sys) method.

   Example: The computer boots from drive C (moderate HPFS or FAT sized
   drive).  Drive D (large HPFS) requires more RAM to check than installed
   in the machine.

     Original IFS statement:

          IFS=C:\OS2\HPFS.IFS /CACHE:2048 /CRECL:32 /AUTOCHECK:CD

     New IFS statement:

          IFS=C:\OS2\HPFS.IFS /CACHE:2048 /CRECL:32 /AUTOCHECK:C /QUIET

     The CALL statement to use is:

          CALL=C:\OS2\CHKDSK.COM D: /C


   The /C option tells CHKDSK to check the drive only if it is "dirty" and
   it needs checking.



   
                                                            New Function  21


                   October 18, 2000 - Warp 3 FixPak XR_W043

   If you need to boot from diskettes to check an HPFS drive, you must have
   the following files on the diskette you wish to run CHKDSK from:

     CHKDSK.COM
     CHKDSK32.DLL
     UHPFS.DLL


   Note: CHKDSK.COM, CHKDSK32.DLL and UHPFS.DLL from FixPak 30 will not work
   on a Warp system with a service level prior to FixPak 29. This is because
   of a new pack program introduced at FixPak 29 level.



   5.10.2 CHKDSK LOG FORMATTER

   CHKDSK creates a binary service log file (chkdsk.log) on the root of the
   drive being checked during autocheck or whenever the /F option is
   invoked.  The previous log file is saved as chkdsk.old. A formatter for
   this log file can be found at:

   ftp://service.boulder.ibm.com/ps/products/os2/fixes/chklogpk.exe


   This is a self extracting ZIP file. Place it in a directory in your path
   and enter CHKLOGPK. This will create the following files:

     message.txt
     msghdr.txt
     pmchklog.exe
     range.txt
     readme


   They should all have a date of 05/14/97 or later (May 14, 1997).

   This is a tool used by OS/2 service to format and view the new CHKDSK log
   entries.  There is no support for this tool. You are welcome to use it
   but if you have problems with it or do not understand the output DO NOT
   contact IBM for assistance as none will be provided.


   5.11 AUTOMATED TRAP SCREEN LOGGING

   Whenever an application program traps, the trap information is (now)
   automatically logged in the POPUPLOG.OS2 file. This is a cumulative file
   that is by default located in the root directory of the bootable
   partition.  Should this file become too large then it may be erased or
   pruned (reduced in size). The system will automatically re-create it if
   it does not exist.


   
                                                            New Function  22


                   October 18, 2000 - Warp 3 FixPak XR_W043

   The TRAPLOG command and SUPPRESSPOPUPS CONFIG.SYS statement may be used
   to control trap screen behavior (see below).


   5.11.1 SUPPRESSPOPUPS

   SUPPRESSPOPUPS=0 will restore behavior to pre-FixPak 29 behavior.  That
   is, to disable logging and to have trap screens displayed unless
   specifically overridden by an application's use of the DosError API.

   SUPPRESSPOPUPS=x: will disable trap screen display for all processes and
   will log trap screens in x:\POPUPLOG.OS2, where x: is a drive or
   partition.

   If SUPPRESSPOPUPS is omitted then the behavior is as described above
   under "Automated Trap Screen Logging".


   5.11.2 TRAPLOG

   The TRAPLOG command allows dynamic control of trap information logging.

   The command syntax is:

          TRAPLOG [x: | NOLOG] [POPUPS | NOPOPUPS]


   where:

   Ž  x: specifies that trap information is to be logged in
       x:\POPUPLOG.OS2, x: being any partition drive letter.
   Ž  NOLOG disables logging of trap information.
   Ž  POPUPS enables the trap information pop-up message (SYS3175).
   Ž  NOPOPUPS disables the trap information pop-up message.



   5.12 TRAPDUMP

   The TRAPDUMP command allows the conditions under which a trap will
   initiate a System Dump to be set dynamically. Prior to Warp 3.0 FixPak
   29, the System Dump setting could only be manipulated from CONFIG.SYS by
   use of the TRAPDUMP statement.

   Use of this command should be made under the direction of service
   personnel.

   Warning: The initiation of a System Dump causes an immediate termination
   of the system without any shutdown. No file system shutdown is performed.
   The system behaves as if a fatal crash has occurred, thus under rare
   circumstances data can be lost.

   
                                                            New Function  23


                   October 18, 2000 - Warp 3 FixPak XR_W043

   The command syntax is:

          TRAPDUMP [[ON] | [OFF] | [R0]] [x:] [/NOCHECK]


   where:

   Ž  ON enables all application and system traps to initiate a System Dump.
   Ž  OFF disables automatic dump initiation.
   Ž  R0 enables only Ring 0 traps to initiate a System Dump.
   Ž  x: specifies the Dump Partition.
   Ž  NOCHECK overrides the system level check for WARP 4.0, since use of
      this command on a system level prior to FixPak 29 is equivalent to the
      SYSDUMP command.



   5.13 SYSDUMP

   The SYSDUMP command forces a System Dump to be initiated, regardless of
   the TRAPDUMP settings. This command is provided for the use of service
   personnel to allow Dump Initiation to be automated through use of a
   command file.

   Warning: The initiation of a System Dump causes an immediate termination
   of the system without any shutdown. No file system shutdown is performed.
   The system behaves as if a fatal crash has occurred thus under rare
   circumstances data can be lost.

   The command syntax is:

          SYSDUMP [/NOPROMPT]


   where:

   Ž  NOPROMPT allows the Dump to proceed without the prompt and response to
      message:

          "Do you want to force a system dump? (Y/N)"




   5.14 OTHER README FILES

   There are other README files containing information you may want to
   review.  All except README.DBG are found on the first FixPak disk and are
   not copied to your system when the Fixpak is installed. README.DBG will
   be copied to the \OS2\INSTALL directory during installation beginning
   with Fixpak 10 and Fixpak 41.

   
                                                            New Function  24


                   October 18, 2000 - Warp 3 FixPak XR_W043

   File           Use

   README2        Problems fixed in each FixPak (APAR list)

   README.CID     Installing FixPaks via CID

   README.REG     Use of the Warp Registry Editor REGEDIT2.EXE

   README.DBG     Tips on debugging OS/2 Warp and details on the latest
                  Serviceability (RAS) Enhancements (3.0 and 4.0).



   5.15 RESERVE DRIVE LETTERS ADDED

   The Reserve Drive Letters feature has been added at Warp FixPak level
   XR_W024 for Uni Processor versions of Warp 3.  It is not included in the
   SMP (Symmetric Multi Processors) version of Warp 3.

   A modification has been made to the OS/2 kernel that will allow the user
   to specify, through a CONFIG.SYS parameter, specific drive letters that
   will not be allocated for local block mode devices during the processing
   of CONFIG.SYS.

   Currently, all versions of OS/2 assign drive letters sequentially
   starting from drive C: for all local devices or disk partitions. Any
   network use of drive letters starts after the last drive letter used for
   local devices/partitions.

   RESERVEDRIVELETTER can be used to force a specific drive letter to be
   allocated to a network drive or a CDROM for example.

   SYNTAX:  RESERVEDRIVELETTER=x, where "x" is letter D thru Z.


   Note: Multiple RESERVEDRIVELETTER statements are allowed but only the
   last one is used.

   During the processing of CONFIG.SYS, OS/2 allocates drive letters for all
   BASEDEV= statements. In general, the only BASEDEV= statements that
   allocate drive letters are those for the Disk Device Driver, which will
   allocate 1 drive letter sequentially for each local disk partition. Three
   local disk partitions would allocate C:,D:,E:.

   After processing BASEDEV= statements, the system will honor the
   RESERVEDRIVELETTER statement(s). If the RESERVEDRIVELETTER statement
   conflicts with any drive letter already assigned to a local disk
   partition, an error message will be generated and that RESERVEDRIVELETTER
   statement will be ignored.



   
                                                            New Function  25


                   October 18, 2000 - Warp 3 FixPak XR_W043

   The next processing occurs for DEVICE= statements.  DEVICE= statements
   for local block mode devices will assign drive letters, starting
   sequentially immediately after the highest drive letter specified in a
   RESERVEDRIVELETTER statement. Examples of local devices which use drive
   letters are CDROM, R/W OPTICAL, TAPE, Virtual Disks (VDISK).

   EXAMPLE: User has 2 local disk partitions, wants the E: drive letter to
   be used as a network drive, has both a CDROM and a R/W optical drive, and
   wants the CDROM drive letter to be K:.

   Specify a RESERVEDRIVELETTER=J statement and insure that the DEVICE=
   statement for the CDROM preceeds the DEVICE= statement for OPTICAL in
   CONFIG.SYS. Note that all drive letters between E and J will be available
   for use by programs or device drivers, which allocate drive letters for
   non-local use like network redirectors.


   5.16 WHAT IS THE SIQ (SINGLE INPUT QUEUE) FEATURE

   The "SIQ" feature is new with FixPak XR_W017. It allows the user to take
   focus away from an application that is monopolizing the message queue.
   When the FixPak is installed, the SIQ feature is disabled (OFF).


   5.16.1 HOW IT WORKS

   When you request a focus change for example, by clicking on another
   application or pressing Ctl+Esc the application that has the focus should
   respond to the message in x milliseconds.  If the application does not
   respond within that time, OS/2 determines that the application is not
   responding to messages and flags the application queue as bad. It then
   switches focus to the desired application.

   OS/2 will monitor the queue marked as bad to see when it does start
   responding to messages. It will mark the queue as good when this occurs.

   To enable the SIQ feature, put a SET PM_ASYNC_FOCUS_CHANGE statement in
   CONFIG.SYS and reboot.

   The parameters to the SET command are:

          SET PM_ASYNC_FOCUS_CHANGE=ON | ON x | OFF

          The default is OFF (disabled).


   To turn it on (enable) put the following in the CONFIG.SYS file and
   reboot:

          SET PM_ASYNC_FOCUS_CHANGE=ON


   
                                                            New Function  26


                   October 18, 2000 - Warp 3 FixPak XR_W043

   To change the timeout value put the following in the CONFIG.SYS file and
   reboot:

          SET PM_ASYNC_FOCUS_CHANGE=ON x

          where x is in milliseconds (default is 2000 (2 seconds))



   If you think you are having problems with SIQ, a way to isolate a problem
   is to raise the timeout to 5000 milliseconds (5 seconds).  If that does
   not help, turn it off.  If there is a SIQ feature problem, this will help
   us (IBM) isolate it.


   5.17 COMMON FILE DIALOG INTERFACE CHANGES

   Beginning with FixPak XR_W017, the Common File Dialog interface has been
   rearranged to improve usability. The changes are:

   Ž  "Type of file" field moved below the Open filename.
   Ž  "Drive" and "Directory" controls were swapped with the "File" control.






























   
                                                            New Function  27


                   October 18, 2000 - Warp 3 FixPak XR_W043

   6.0 CORRECTIVE SERVICE FACILITY



   6.0.1 REQUIRED CSF LEVEL

   You must use release level f.143 or later of the OS/2 Corrective Service
   Facility to install this FixPak.  Check the BUILD.LVL file for the level
   you are using.  If it does not have a BUILD.LVL file then it is old and
   cannot be used.


   6.0.2 WHERE YOU CAN FIND CSF CODE

   The latest Corrective Service Facility code is available from:

   ftp://service.boulder.ibm.com/ps/products/os2/fixtool/

   Select the required language then the latest fixtool release (CS?140 at
   the time this Fixpak was released).

   The .TXT file has instructions.  The .EXE is a self-extracting ZIP file
   that contains the CSF code.  See the READ.ME file contained in .EXE for
   information on how to use the new CSF.


   6.0.3 CREATING FIXPAK DISKETTES

   Use LOADDSKF.EXE to create the diskettes. For each disk image, place a
   2MB HD (1.44MB formatted) diskette in A:.

   Warning: DO NOT use a 1MB (720KB formatted) diskette because you might
   have problems trying to install this FixPak.

   For each diskette image in the FixPak, do the following:

   Enter LOADDSKF XR_W043.?DK A: /F  (? can be 1 through 9, A through Z).

   Label the diskette as

         FixPak XR_W043
   Corrective Service Diskette ?
          (CSF DISK ?)


   Note: For diskette images ADK through ZDK (if they exist), use the
   numbers 10 through 36.





   
                                             Corrective Service Facility  28


                   October 18, 2000 - Warp 3 FixPak XR_W043

      Examples:
        XR_W043.ADK = Corrective Service Diskette 10 (CSF DISK 10)
        XR_W043.BDK = Corrective Service Diskette 11 (CSF DISK 11)
        XR_W043.CDK = Corrective Service Diskette 12 (CSF DISK 12)
        XR_W043.DDK = Corrective Service Diskette 13 (CSF DISK 13)
      etc.














































   
                                             Corrective Service Facility  29


                   October 18, 2000 - Warp 3 FixPak XR_W043

   7.0 RELOCATED OS/2 FILE SUPPORT

   This FixPak will service directories based on the location of supported
   SYSLEVEL.OS2 and SYSLEVEL.MPM files.  Please check your system to make
   sure extra copies of these files are not located in directories other
   than:

     \OS2\INSTALL\SYSLEVEL.OS2 on the boot drive of your OS/2 partition(s)
     \MMOS2\INSTALL\SYSLEVEL.MPM on any partition


   If additional copies of these files are found in other locations on your
   hard disk then CSF will try to service files as follows:

   For SYSLEVEL.OS2

     ..\..\   all files in a directory two levels above (toward the root).
              This should be the root directory of your boot drive.
     ..\*     all files in a directory one level above (toward the root) and
              all subdirectories below. This should be the OS2 directory and
              subdirectories.


   For SYSLEVEL.MPM

     ..\*     all files in a directory one level above (toward the root) and
              all subdirectories below. This should be the MMOS2 directory and
              subdirectories.


   If you have moved OS/2 files or directories, do the following in order to
   have them serviced:

   1. Create a file named USERDIRS.OS2 in the \OS2\INSTALL directory of the
      OS\2 Warp partition to be serviced.

      In this file, place the full path to the directory you want to be
      serviced. Examples would be:

        C:\JSI\*
        D:\JSI\SH\*


      Be sure to include the trailing * (asterisk) after the last backslash.

   Note: Leave this file for any future OS/2 Warp FixPaks you might apply.






   
                                             Relocated OS/2 file support  30


                   October 18, 2000 - Warp 3 FixPak XR_W043

   8.0 LAN SERVER/WARP SERVER REMOTE IPL CONSIDERATIONS

   The utility mentioned in this section is on the last FixPak disk.

   Ž  UPDTRIPL.EXE

   To support the OS/2 3.0 DAX function, the following updates must be made
   to the Remote IPL(RIPL) control files:

   Ž  Update the d:\IBMLAN\RPL\FITS\DEFALT30.FIT file to add the following
      entry to the end of the file:

        Z:\*.DAT                                OS2.30


   Ž  For each RIPL client that is defined to boot OS/2 3.0, update the
      d:\IBMLAN\RPL\FITS\client.FIT file to add the following entry to the
      end of the file:

        Z:\*.DAT                                OS2.30

        Note: In the file name client is the name of the RIPL machine.


   Ž  For each RIPL client that is defined to boot OS/2 3.0,  run the
      utility UPDTRIPL.EXE to update the client CONFIG.SYS and OS2.INI
      files.  You must specify the fully qualified path for both files as
      parameters to UPDTRIPL.EXE.

      The syntax of UPDTRIPL is:

      UPDTRIPL client_config_sys  client_os2_ini  <client_boot_drive>

      Each client copy of OS2.INI will be located in the
      d:\IBMLAN\RPLUSER\client\OS2 directory.  The os2.INI path parameter
      for UPDTRIPL.EXE will be d:\IBMLAN\RPLUSER\client\OS2\OS2.INI.

      Each client copy of CONFIG.SYS can be in two different directories,
      depending on what type of video support the client is configured to
      use.  The two possibilites are:

      1. If the client is configured for SVGA or S3SVGA support, the
         CONFIG.SYS file will be located in the d:\IBMLAN\RPLUSER\client
         directory.

         Note: There will be a CONFIG.SYS file in the
         d:\IBMLAN\RPL\MACHINES\client directory.  However, it is not used
         when the client is configured for SVGA or S3SVGA support.
      2. If the client is configured for any other video type, the
         CONFIG.SYS file will be located in the
         d:\IBMLAN\RPL\MACHINES\client directory.

   
                        LAN Server/Warp Server Remote IPL Considerations  31


                   October 18, 2000 - Warp 3 FixPak XR_W043

         If you are not sure which video type the client is configured to
         use, do the following to determine which CONFIG.SYS the client is
         using:
         a. Edit the d:\IBMLAN\RPL\FITS\client.FIT file.
         b. Search for the line that starts with Z:\CONFIG.SYS (assumes that
            the client is using the default boot drive of Z:).
         c. If the second field (target file name) is
            MACHINES\client\CONFIG.SYS, the path is
            d:\IBMLAN\RPL\MACHINES\client\CONFIG.SYS.

            If the second field is \\servername\WRKFILES\client\CONFIG.SYS,
            the path is d:\IBMLAN\RPLUSER\client\CONFIG.SYS.

            Note: servername is the LAN server name.
   Ž  Run the UPDTRIPL.EXE utility and update the default OS/2 3.0
      CONFIG.SYS and OS2.INI files. The actual file names to update are
      d:\IBMLAN\RPL\MACHINES\DEFALT30\CONFIG.DEF and
      d:\IBMLAN\RPLUSER\DEFALT30\OS2\OS2.INI.
   Ž  Check the Access Control Profile (ACP) for the
      C:\IBMLAN\RPL\OS2.30\LANGUAGE directory. The RPLGROUP ID should have
      RX access.  Follow these steps to check the ACP:
      1. Logon as administrator .
      2. Open the drives folder under OS/2 system
      3. Find the OS2.30\LANGUAGE folder under \IBMLAN\RPL
      4. Select (Single-click with Left mouse button) the OS2.30\LANGUAGE
         folder
      5. From the pop-up menu (Single click with Right mouse button), select
         "Manage Access"
      6. Click on the Permissions Tab .

       If the RPLGROUP ID does not have RX permissions,  do the following:
      1. Click on the Add button and select RPLGROUP, and click on OK
      2. Add permissions Read and Execute and click on Change.
      3. Click on Set (Bottom of the window)
      4. Click on OK to propagate this Access Control Profile to all of the
         resource's subdirectories.
















   
                        LAN Server/Warp Server Remote IPL Considerations  32


                   October 18, 2000 - Warp 3 FixPak XR_W043

   9.0 INSTALLATION PROCESS



   9.1 BEFORE INSTALLATION

   Before installing any FixPak, run CHKDSK /F against all drives on your
   system to correct any file system errors that might be present. You
   cannot do this while OS/2 is active. You must shut down and run CHKDSK by
   one of the following methods:

   Ž  Boot from your Installation and DISK 1 diskettes you used to install
      OS/2 with.  If your file system is HPFS, then put the diskette with
      CHKDSK and UHPFS.DLL on it in your A: drive before issuing the CHKDSK
      command.
   Ž  Boot from the Utilities disk you created via the "Create Utility
      Diskettes" icon in the System Setup folder.
   Ž  Boot from a different OS/2 partition.



   9.2 METHOD 1: INSTALL FROM BOOTED OS/2 PARTITION.

   This method allows you to select the products (partitions) to be
   serviced.

   This is the method you should use if you have more than one OS/2
   partition and want to control which one is serviced.

   Note: You can use a diskette drive other than A: with this method. If
   your 3.5" diskette drive is B:, use B: where A: is mentioned in the
   following steps.  (this method only).

   1. Insert CSF DISK Diskette 1 in drive A.
   2. Open an OS/2 window or full-screen session.
   3. Type A:\SERVICE and press the Enter key.

      Note: You could also use the "Drives" object for A: and double click
      on the "SERVICE.EXE" Icon to start the install.
   4. Follow the displayed instructions. When prompted to insert Corrective
      Service Diskette 1 (not CSF DISK Diskette 1), place FixPak XR_W043
      Corrective Service Diskette 1 in drive A. Repeat for the rest of the
      FixPak disks when requested to do so.

      Note: It can take a considerable length of time for the Corrective
      Service Facility to scan your hard disk for serviceable files. In some
      cases, it has taken as long as 40 minutes. Please be patient and allow
      this process to complete.
   5. If this is the first OS/2 Warp FixPak you have applied to this system,
      then enter the path to the ARCHIVE directory where a copy of replaced
      files will be stored (for example, D:\ARCHIVE).

   
                                                    Installation Process  33


                   October 18, 2000 - Warp 3 FixPak XR_W043


      Note: This ARCHIVE directory is not related to the ARCHIVES directory
      built into OS/2 Warp 3.0. Please specify a different path.  You must
      specify a different ARCHIVE directory for each product to be serviced.

      If this is not the first OS/2 Warp FixPak, then enter the path to the
      BACKUP directory where a copy of replaced files will be stored (for
      example, D:\BACKUP).

      Note: You must specify a different BACKUP directory for each product
      to be serviced.

      For either case, make sure there is sufficient space available on the
      drive you specify. Even though these files are kept in compressed
      (PACK2) format, they require between 7 and 12 MB of disk space.
   6. Click on "OK".
   7. You will see an "Application in use" dialog box showing a list of
      locked files that cannot be serviced while the system is running.  You
      are given two choices - to Continue or Reboot. Select Continue.
   8. During the installation process you might see messages about
      Archiving, Updating and Deferring service.
      Ž  Archiving saves a compressed copy of the original file in the
         ARCHIVE or BACKUP path you specified.
      Ž  Updating means the original files are replaced with the new ones
         from this FixPak.
      Ž  Deferring service means the file to be updated is currently in use
         by the system and cannot be updated. The new files from the FixPak
         are placed in unpacked format in the \IBMCSFLK\FIX directory on the
         drive with the most free space.  They are processed by the locked
         file device driver during reboot after you shut down the system.
   9. Select NO for a redisplay of the "Product List" after the first part
      of the FixPak application process has completed if this message is
      displayed.
   10.Click Cancel and Exit to close the Corrective Service Facility window
      if necessary.
   11.Shut down and reboot your system.

      You will see the following during reboot of the system if you applied
      service to the OS/2 partition you were booted from.

      The locked file driver is loaded.

             Processing locked files

             Processing complete


      The system will do one automatic reboot after the Locked File Device
      Driver has completed.



   
                                                    Installation Process  34


                   October 18, 2000 - Warp 3 FixPak XR_W043

   9.3 METHOD 2: BOOT FROM CORRECTIVE SERVICE DISK 1.

   This method does not prompt the user for any information. No interaction
   with the user takes place other than requests to put the next diskette in
   drive A.  All serviceable partitions on your system will be updated
   automatically. Be especially careful of extra SYSLEVEL.OS2 or
   SYSLEVEL.MPM files when using this method because they can cause CSF to
   apply service to directories you do not want serviced.

   1. Shut down your OS/2 system.
   2. Insert CSF DISK Diskette 1 in drive A.
   3. Press Ctrl+Alt+Del to boot the disk in drive A.

   Service will be applied to ALL partitions that contain a version of OS/2
   that is supported by this FixPak. See the section "FixPak Corrective
   Service Notes" for the CSD levels this FixPak applies to.

   Note: It can take a considerable length of time for the Corrective
   Service Facility to scan your hard disk for serviceable files. In some
   cases it has taken as long as 40 minutes. Please be patient and allow
   this process to complete.


   9.4 ADDITIONAL CORRECTIVE SERVICE FACILITY INFORMATION

   Additional information on the Corrective Service Facility is available
   from the README.INF file on the first Corrective Service Facility disk.
   To view this file, place CSF disk 1 in drive A and enter VIEW
   A:\README.INF.























   
                                                    Installation Process  35


                   October 18, 2000 - Warp 3 FixPak XR_W043

   10.0 CSD LEVEL OF SYSLEVEL.OS2

   The Current CSD level field of the SYSLEVEL.OS2 file in each serviced
   partition will be updated with the name of the FixPak when it is applied.

   This is a major change from previous CSF releases.  The Prior CSD level
   field will be left asis.  This means when you use the SYSLEVEL command to
   look at the release levels of products on your system, you will see
   something like the following for SYSLEVEL.OS2.

   Before a FixPak is applied using the F.138B CSF build (or later) to a
   Warp Connect system.

      E:\OS2\INSTALL\SYSLEVEL.OS2
      IBM OS/2 Base Operating System
      Version 3.0      Component ID 562274700
      Type 0C
      Current CSD level: XR03003
      Prior   CSD level: XR03003


   After a FixPak is applied using the F.138B CSF build (or later) to a Warp
   Connect system.

      E:\OS2\INSTALL\SYSLEVEL.OS2
      IBM OS/2 Base Operating System
      Version 3.0      Component ID 562274700
      Type 0C
      Current CSD level: XR0W040
      Prior   CSD level: XR03003


   All fix information is recorded in SERVICE.LOG. Look at the file

      \OS2\INSTALL\SERVICE.LOG


   on your boot drive for information relating to the installation of
   FixPaks on your system.

   Additionally, you can use the VER /R command to see the current revision
   of OS/2 installed.  The response will look like the following for this
   FixPak:

   The Operating System/2 Version is 3.00
   Revision n.nnn


   The first page of this document has a line that looks like:



   
                                               CSD level of SYSLEVEL.OS2  36


                   October 18, 2000 - Warp 3 FixPak XR_W043

   Build Level: n.nnn


   That is the number you should see for this FixPak when you issue the VER
   /R command.


   10.0.1 NEW SYSLEVEL.FPK

   A SYSLEVEL.FPK file has been added to all Warp 3 FixPaks, beginning with
   XR_W032. It is titled "OS/2 Warp 3 Service Level". It contains the name
   of the currently installed FixPak in both the Current and Previous CSD
   level fields and is located in the same directory the SYSLEVEL.OS2 file
   is located in which should be \OS2\INSTALL.

   The easiest way to look at SYSLEVEL information is to use the SYSLEVEL
   command and redirect the output to a file then edit the file and search
   for SYSLEVEL.FPK.


































   
                                               CSD level of SYSLEVEL.OS2  37


                   October 18, 2000 - Warp 3 FixPak XR_W043

   11.0 FIXPAK CORRECTIVE SERVICE LEVELS AND DISK LAYOUTS

   Build Level: 8.267

   Product location on CSD:  A:\FIX\OS2.1
   Product name:  "IBM OS/2 Base Operating System"
   Standard Edition  3.01
   Fixpak name:   XR_W043_   (Country = Generic)
   Pre-requisite CSD Level:  XR_3005_
   System Id:  1000
   Component Id:  562274700
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM OS/2 Base Operating System"
   Standard Edition  3.02
   Fixpak name:   XR_W043_   (Country = Generic)
   Pre-requisite CSD Level:  XR_3006_
   System Id:  1000
   Component Id:  5639A5500
   Archive is ON for this product.
   ________________________________________________________________________

   Default directories:

           ..\..\
           ..\*
           ..\..\VT
           ..\..\VT\*
           ..\..\PSFONTS
           ..\..\PSFONTS\*
           ..\..\LANGUAGE
           ..\..\LANGUAGE\*
   Will create the following directories
      ..\..\OS2\BOOK   Stub File:  @BOOKDIR

      ..\..\OS2\BOOT   Stub File:  @BOOTDIR

      ..\..\LANGUAGE\CODEPAGE   Stub File:  @CDEPDIR

      ..\..\OS2\DLL   Stub File:  @DLLDIR

      ..\..\OS2\HELP   Stub File:  @HELPDIR

      ..\..\OS2\INSTALL   Stub File:  @INSTDIR

      ..\..\OS2\APPS   Stub File:  @APPSDIR

      ..\..\LANGUAGE\KEYBOARD   Stub File:  @KEYBDIR

      ..\..\LANGUAGE\LOCALE   Stub File:  @LOCLDIR


   
                       FixPak Corrective Service levels and disk layouts  38


                   October 18, 2000 - Warp 3 FixPak XR_W043

      ..\..\OS2\MDOS   Stub File:  @MDOSDIR

      ..\..\OS2   Stub File:  @OS2DIR

      ..\..\OS2\SYSTEM\PMDF   Stub File:  @PMDFDIR

      ..\..\OS2\SYSTEM\RAS   Stub File:  @RASDIR

      ..\..\OS2\SYSTEM   Stub File:  @SYSTDIR

      ..\..\OS2\SYSTEM\TRACE   Stub File:  @TRACDIR


   Files contained in Fixpak for product:

   Filename      Name on CSD   Disk#  Date        Time   Size     Checksum
   ------------  ------------  -----  ----------  -----  -------  --------
   AA.KBL        AA.KB_         11    12/02/1999  14:19     1200  41C9ECA1
   AA470.KBL     AA470.KB_      11    12/02/1999  14:19     1212  7FBC26F6
   ARACONV.EXE   ARACONV.EX_     9    11/23/1999  20:12    62151  F784F7D0
   ARCINST.EXE   ARCINST.EX_    10    07/25/2000  00:06    19798  85C8158D
   ARCRECOV.EXE  ARCRECOV.EX_   10    07/25/2000  00:07    21871  D6E7ECCB
   ASIACOL.DLL   ASIACOL.DL_     5    12/02/1999  14:20   158758  3988EF24
   BA.KBL        BA.KB_         11    12/02/1999  14:19      980  CAEB4F87
   BACKUP.EXE    BACKUP.EX_     10    07/24/2000  22:17    32736  657A9C9D
   BDCALLS.DLL   BDCALLS.DL_    10    01/08/1998  18:09    37594  F7D833A0
   BDIME.DLL     BDIME.DL_      10    04/13/1999  08:18    33239  BC50FC0E
   BE.KBL        BE.KB_         11    12/02/1999  14:19      972  B9CF6F4D
   BG.KBL        BG.KB_         11    12/02/1999  14:19     1152  3B11B14E
   BG241.KBL     BG241.KB_      11    12/02/1999  14:19     1372  B79DBAB4
   BLDLEVEL.EXE  BLDLEVEL.EX_   11    07/24/2000  23:37    21523  ED40532C
   BOOT.COM      BOOT.CO_       10    07/24/2000  22:38    43056  CB48623E
   BOOTDISK.EXE  BOOTDISK.EX_    9    07/25/2000  00:47    48777  E89F5429
   BR.KBL        BR.KB_         11    12/02/1999  14:19      932  12509F8B
   BR274.KBL     BR274.KB_      11    12/02/1999  14:19      852  875F122C
   BVHWNDW.DLL   BVHWNDW.DL_    11    02/17/1998  15:37    14233  665B49D8
   BVSCALLS.DLL  BVSCALLS.DL_   11    08/26/1998  01:32      512  4062D2D3
   BY.KBL        BY.KB_         11    12/02/1999  14:19     1292  7E1B2D68
   CA.KBL        CA.KB_         11    12/02/1999  14:19     1214  153AD27D
   CALC.EXE      CALC.EX_       10    07/19/1999  16:14    43056  A1BB49B5
   CALENDAR.EXE  CALENDAR.EX_    9    07/19/1999  16:15    59808  65473CF6
   CARDFILE.EXE  CARDFILE.EX_    9    07/19/1999  16:16    93184  8AB13196
   CARDINFO.DAT  CARDINFO.DA_    2    12/07/1998  10:00    29787  BD0C262B
   CDFS.IFS      CDFS.IF_       10    07/24/2000  21:37    45151  9D7BDB8A
   CDFS.TDF      CDFS.TD_       11    07/24/2000  21:37     2113  81DC2068
   CDROM.TBL     CDROM.TB_      11    03/12/1997  17:33     3658  2E96808F
   CF.KBL        CF.KB_         11    12/02/1999  14:19      956  B1186AE5
   CHARMAP.EXE   CHARMAP.EX_    11    07/19/1999  16:28    22016  6022A98C
   CHKDSK.COM    CHKDSK.CO_      9    07/24/2000  22:21    68656  9453C617
   CHKDSK.SYS    CHKDSK.SY_     11    08/24/2000  09:38      762  8FBB6856
   CHKDSK32.DLL  CHKDSK32.DL_    7    08/18/2000  15:31   170023  B8765BDE

   
                       FixPak Corrective Service levels and disk layouts  39


                   October 18, 2000 - Warp 3 FixPak XR_W043

   CHKDSK32.EXE  CHKDSK32.EX_   11    08/18/2000  15:02     6417  DDDF2ADB
   CLDAPI.DLL    CLDAPI.DL_     10    07/24/2000  23:52    22217  C0E59D60
   CLIPBRD.EXE   CLIPBRD.EX_    11    07/19/1999  16:16    18496  B3F5949C
   CLOCK.EXE     CLOCK.EX_      11    07/19/1999  16:17    16400  E74F144F
   CLOCK01.SYS   CLOCK01.SY_    11    08/14/2000  19:15     4560  C92593EC
   CLOCK02.SYS   CLOCK02.SY_    11    08/14/2000  19:15     4318  FBE906A4
   CMD.EXE       CMD.EX_         3    07/24/2000  22:26    71556  A506F0B8
   COMM.DRV      COMM.DR_       11    07/19/1999  18:10     9552  353CF5F2
   COMMAND.COM   COMMAND.CO_     9    07/24/2000  22:24    53014  66A8CCDB
   COMMDLG.DLL   COMMDLG.DL_     8    07/19/1999  16:12    87072  B987A798
   COMMONA.DSP   COMMONA.DS_    11    03/27/1998  14:21      429  CD1C47BE
   CONTROL.EXE   CONTROL.EX_    11    07/19/1999  16:54    15856  CFA1BC10
   COUNTRY.SYS   COUNTRY.SY_    11    07/24/2000  22:53    50932  CD0A6677
   COUR.OFM      COUR.OF_       11    01/13/1998  14:37     4236  61F7551D
   COUR.PFB      COUR.PF_        5    01/13/1998  14:37   112702  F4783159
   COUR.PFM      COUR1.PF_      11    01/13/1998  14:37      674  EB15B168
   COURB.OFM     COURB.OF_      11    01/13/1998  14:37     4246  1F31D3E4
   COURB.PFB     COURB.PF_       5    01/13/1998  14:37   116938  114C7222
   COURB.PFM     COU1.PF_       11    01/13/1998  14:37      679  1EF9C6BB
   COURBI.OFM    COURBI.OF_     11    01/13/1998  14:37     4260  8CFE6AF3
   COURBI.PFB    COURBI.PF_      5    01/13/1998  14:37   112484  875E9829
   COURBI.PFM    COURB1.PF_     11    01/13/1998  14:37      685  D0390DEF
   COURI.OFM     COURI.OF_      11    01/13/1998  14:37     4251  4253A3B8
   COURI.PFB     COURI.PF_       5    01/13/1998  14:37   113244  48B65D0F
   COURI.PFM     COUR2.PF_      11    01/13/1998  14:37      681  A6EEB717
   COURIER.FON   COURIER.FO_    10    01/19/1998  13:35   104183  CE3E3300
   CPG01256.TBL  CPG01256.TB_   11    11/22/1999  12:17    27264  A5C721BD
   CZ.KBL        CZ.KB_         11    12/02/1999  14:19     1014  B5779D23
   DDEML.DLL     DDEML.DL_      10    07/19/1999  16:11    36864  0FC24679
   DDINSTAL.EXE  DDINSTAL.EX_    9    07/24/2000  22:56    35879  8539CF2C
   DE.KBL        DE.KB_         11    12/02/1999  14:19      958  96E0DDA3
   DE453.KBL     DE453.KB_      11    12/02/1999  14:19     1354  B6DDE2E1
   DISPLAY.DLL   DISPLAY.DL_     9    07/10/2000  13:48    44198  48E36628
   DK.KBL        DK.KB_         11    12/02/1999  14:19      928  46C631AF
   DMCOLOR.DLL   DMCOLOR.DL_    11    07/19/1999  17:20    18480  B716CA14
   DMQSPROF.DLL  DMQSPROF.DL_    9    07/26/1999  20:55    43278  A37752D3
   DRWATSON.EXE  DRWATSON.EX_   10    07/19/1999  17:05    26864  2F1B8E14
   DSPINSTL.EXE  DSPINSTL.EX_    6    07/24/2000  23:47   112216  358BAA09
   DSPRES.DLL    DSPRES2.DL_     4    01/19/1998  13:35   250598  F6022627
   DSPRES.DLL    DSPRES1.DL_     4    01/19/1998  13:35   250598  F6022627
   DSPRES.DLL    DSPRES.DL_      4    01/19/1998  13:35   250598  F604CE27
   DTRACE.DOC    DTRACE.DO_     10    01/07/1998  17:11    75371  761E5F8B
   DTRACE.EXE    DTRACE.EX_      9    07/24/2000  19:56    48906  AED7058C
   E.EXE         E.EX_           9    07/24/2000  22:15    48389  EA061208
   EAUTIL.EXE    EAUTIL.EX_     10    07/24/2000  22:38    37984  F22463FC
   EE.KBL        EE.KB_         11    12/02/1999  14:19      932  ACF9C974
   EJECT.EXE     EJECT.EX_      10    01/14/1998  16:27    25649  5A75A5C8
   EL.KBL        EL.KB_         11    12/02/1999  14:19     1396  D4F7753C
   EL220.KBL     EL220.KB_      11    12/02/1999  14:19     1428  DD7C28CB
   EL459.KBL     EL459.KB_      11    12/02/1999  14:19     1372  B9F1C4D2
   ES.KBL        ES.KB_         11    12/02/1999  14:19      920  9E1D8E87

   
                       FixPak Corrective Service levels and disk layouts  40


                   October 18, 2000 - Warp 3 FixPak XR_W043

   EXPAND.EXE    EXPAND.EX_     10    07/19/1999  16:07    25432  C8750CF8
   FDISK.COM     FDISK.CO_       7    07/24/2000  21:46   113658  E3D7E1B2
   FDISKPM.DLL   FDISKPM.DL_    11    03/24/1998  16:10     8244  08483FBF
   FDISKPM.EXE   FDISKPM.EX_     8    07/24/2000  21:46    63043  ED274E45
   FI.KBL        FI.KB_         11    12/02/1999  14:19      940  6D873B78
   FINSTALL.DLL  FINSTALL.DL_    6    07/19/1999  17:26   200368  11980150
   FORMAT.COM    FORMAT.CO_      9    07/24/2000  22:47    69920  90976D55
   FR.KBL        FR.KB_         11    12/02/1999  14:19      950  2F060403
   FSFILTER.SYS  FSFILTER.SY_   11    07/24/2000  22:59    12988  428292C1
   GDI.EXE       GDI.EX_         4    07/19/1999  16:42   225744  FC21FFD9
   GRADD.SYS     GRADD.SY_      11    05/15/2000  16:23     2754  05B49EB1
   GRE2VMAN.DLL  GRE2VMAN.DL_   11    08/06/2000  12:13    20653  147372EC
   HARDERR.EXE   HARDERR.EX_    11    07/24/2000  21:52     9416  D02B9D05
   HELPMGR.DLL   HELPMGR.DL_     4    07/24/2000  22:43   175874  7D1CA539
   HELPMSG.EXE   HELPMSG.EX_    10    07/24/2000  22:47    36256  5C784A59
   HELV.FON      HELV.FO_        6    01/19/1998  13:36   264425  4DFE4FF3
   HELV.OFM      HELV.OF_       11    03/12/1998  09:41     4865  E6B9D229
   HELV.PFB      HELV.PF_        6    03/12/1998  09:41   101942  076D61BB
   HELV.PFM      HEL1.PF_       11    03/12/1998  09:41     1096  6F22965A
   HELVB.OFM     HELVB.OF_      11    03/12/1998  09:41     4857  C06526BD
   HELVB.PFB     HELVB.PF_       6    03/12/1998  09:41   104404  D1A162E1
   HELVB.PFM     HELV1.PF_      11    03/12/1998  09:41     1089  84484DE1
   HELVBI.OFM    HELVBI.OF_     11    03/12/1998  09:41     4859  F81293F7
   HELVBI.PFB    HELVBI.PF_      6    03/12/1998  09:41   105074  CEC8B328
   HELVBI.PFM    HELVB1.PF_     11    03/12/1998  09:41     1087  0655029D
   HELVI.OFM     HELVI.OF_      11    03/12/1998  09:41     4844  499A0362
   HELVI.PFB     HELVI.PF_       6    03/12/1998  09:41   103996  73AEF6AC
   HELVI.PFM     HELV2.PF_      11    03/12/1998  09:41     1079  A1475D84
   HPFS.IFS      HPFS.IF_        7    08/24/2000  09:41   144450  4F8FEB3E
   HPFS.TDF      HPFS.TD_       11    08/24/2000  09:41     1620  1DAFFFA7
   HR.KBL        HR.KB_         11    12/02/1999  14:19      982  F9ACEEBA
   HU.KBL        HU.KB_         11    12/02/1999  14:19     1006  C7C7BFEE
   IBM1004       IBM1004.___    11    12/02/1999  14:12     3584  7FAB8F9A
   IBM1006       IBM1006.___    11    12/02/1999  14:12     3040  A9881646
   IBM1008       IBM1008.___    11    12/02/1999  14:12     2816  98C46AD8
   IBM1025       IBM1025.___    11    12/02/1999  14:12     2560  A433126E
   IBM1026       IBM1026.___    11    12/02/1999  14:12     2560  E64DA7D4
   IBM1027       IBM1027.___    11    12/02/1999  14:12     2304  5D7AF143
   IBM1028       IBM1028.___    11    12/02/1999  14:12     3072  599DF53B
   IBM1038       IBM1038.___    11    12/02/1999  14:12     4608  47438A35
   IBM1041       IBM1041.___    11    12/02/1999  14:12     3296  87214004
   IBM1043       IBM1043.___    11    12/02/1999  14:12     3040  3E696709
   IBM1046       IBM1046.___    11    12/02/1999  14:12     3040  DF209620
   IBM1047       IBM1047.___    11    12/02/1999  14:12     2304  5ABDADBB
   IBM1051       IBM1051.___    11    12/02/1999  14:12     3296  2FAFD338
   IBM1088       IBM1088.___    11    12/02/1999  14:12     3552  6597710E
   IBM1089       IBM1089.___    11    12/02/1999  14:12     2560  2AA878BA
   IBM1092       IBM1092.___    11    12/02/1999  14:12     4832  1A30D736
   IBM1097       IBM1097.___    11    12/02/1999  14:12     3040  C5F3B6F2
   IBM1098       IBM1098.___    11    12/02/1999  14:12     4576  ECC99645
   IBM1112       IBM1112.___    11    12/02/1999  14:12     2528  EC54FF2C

   
                       FixPak Corrective Service levels and disk layouts  41


                   October 18, 2000 - Warp 3 FixPak XR_W043

   IBM1114       IBM1114.___    11    12/02/1999  14:12     3552  271C28B0
   IBM1115       IBM1115.___    11    12/02/1999  14:12     3296  EA0A2457
   IBM1116       IBM1116.___    11    12/02/1999  14:12     3808  BD0A0FFF
   IBM1117       IBM1117.___    11    12/02/1999  14:12     3552  3E16B694
   IBM1118       IBM1118.___    11    12/02/1999  14:12     4320  876D28FF
   IBM1119       IBM1119.___    11    12/02/1999  14:12     4096  44C1FB27
   IBM1122       IBM1122.___    11    12/02/1999  14:12     2560  86E90FDC
   IBM1123       IBM1123.___    11    12/02/1999  14:12     2528  6C07803F
   IBM1124       IBM1124.___    11    12/02/1999  14:12     2528  98A6A477
   IBM1125       IBM1125.___    11    12/02/1999  14:12     4320  4929BB62
   IBM1131       IBM1131.___    11    12/02/1999  14:12     4320  41CEE2D2
   IBM1200       IBM1200.___    11    12/02/1999  14:12     2784  359D78D5
   IBM1207       IBM1207.___    11    12/02/1999  14:12      704  0EDFF9F3
   IBM1208       IBM1208.___    11    12/02/1999  14:12      720  9BAC6045
   IBM1250       IBM1250.___    11    12/02/1999  14:12     3552  E5F918EF
   IBM1251       IBM1251.___    11    12/02/1999  14:12     3328  82759905
   IBM1252       IBM1252.___    11    12/02/1999  14:12     3552  9E4CF21E
   IBM1253       IBM1253.___    11    12/02/1999  14:12     3552  CAC6863D
   IBM1254       IBM1254.___    11    12/02/1999  14:12     3552  6E1D9E60
   IBM1255       IBM1255.___    11    12/02/1999  14:12     3808  D4DB82B0
   IBM1256       IBM1256.___    11    12/02/1999  14:12     4320  87492B76
   IBM1257       IBM1257.___    11    12/02/1999  14:12     3296  71DAE5AE
   IBM1275       IBM1275.___    11    12/02/1999  14:12     5600  E5D0DA17
   IBM1276       IBM1276.___    11    12/02/1999  14:12     3072  EC090CD0
   IBM1277       IBM1277.___    11    12/02/1999  14:12     2816  50AEF570
   IBM1280       IBM1280.___    11    12/02/1999  14:12     4832  679B7A30
   IBM1281       IBM1281.___    11    12/02/1999  14:12     5344  DB2812A0
   IBM1282       IBM1282.___    11    12/02/1999  14:12     5120  BD286894
   IBM1283       IBM1283.___    11    12/02/1999  14:12     4832  DA04CBA8
   IBM1381       IBM1381.___     8    12/02/1999  14:12   109792  FA0FD3BB
   IBM1383       IBM1383.___     8    12/02/1999  14:12   127344  42D69E6B
   IBM1386       IBM1386.___     4    12/02/1999  14:12   125200  1515092C
   IBM259        IBM259.___     11    12/02/1999  14:12     4864  46730DBB
   IBM273        IBM273.___     11    12/02/1999  14:12     2304  1DB8EBEB
   IBM277        IBM277.___     11    12/02/1999  14:12     2304  E20FE11A
   IBM278        IBM278.___     11    12/02/1999  14:12     2304  0B4EEC3E
   IBM280        IBM280.___     11    12/02/1999  14:12     2272  EB03021A
   IBM282        IBM282.___     11    12/02/1999  14:12     2272  B5CBF4B5
   IBM284        IBM284.___     11    12/02/1999  14:12     2304  BE576FC1
   IBM285        IBM285.___     11    12/02/1999  14:12     2304  89BF65BD
   IBM290        IBM290.___     11    12/02/1999  14:12     2272  519B5927
   IBM293        IBM293.___     11    12/02/1999  14:12     3040  C02BE129
   IBM297        IBM297.___     11    12/02/1999  14:12     2272  107DE98C
   IBM2TI1.EXE   IBM2TI1.EX_    11    05/13/1996  21:15     9886  E248A23F
   IBM2TI1.SYS   IBM2TI1.SY_    11    05/13/1996  21:15     9886  E251A23F
   IBM300        IBM300.___      8    12/02/1999  14:12    94432  97C181F2
   IBM301        IBM301.___      9    12/02/1999  14:12    83168  3979EBA1
   IBM361        IBM361.___     11    12/02/1999  14:12     3584  8AD912EE
   IBM363        IBM363.___     11    12/02/1999  14:12     4864  D657D238
   IBM367        IBM367.___     11    12/02/1999  14:12     2016  846429C5
   IBM37         IBM37.___      11    12/02/1999  14:12     2304  E3CB40FF

   
                       FixPak Corrective Service levels and disk layouts  42


                   October 18, 2000 - Warp 3 FixPak XR_W043

   IBM382        IBM382.___     11    12/02/1999  14:12     3584  5489972C
   IBM383        IBM383.___     11    12/02/1999  14:12     3584  1C23D7D0
   IBM385        IBM385.___     11    12/02/1999  14:12     3584  8392F43A
   IBM386        IBM386.___     11    12/02/1999  14:12     3584  D9E3DFB8
   IBM387        IBM387.___     11    12/02/1999  14:12     3584  866E8F16
   IBM388        IBM388.___     11    12/02/1999  14:12     3584  714861F0
   IBM389        IBM389.___     11    12/02/1999  14:12     3584  85403B11
   IBM391        IBM391.___     11    12/02/1999  14:12     3584  5EF82797
   IBM392        IBM392.___     11    12/02/1999  14:12     3584  BDECF0ED
   IBM393        IBM393.___     11    12/02/1999  14:12     3584  E30AC396
   IBM394        IBM394.___     11    12/02/1999  14:12     3584  CE4856EB
   IBM395        IBM395.___     11    12/02/1999  14:12     3584  EC75516B
   IBM420        IBM420.___     11    12/02/1999  14:12     3040  9731D534
   IBM424        IBM424.___     11    12/02/1999  14:12     2528  DA18519E
   IBM437        IBM437.___     11    12/02/1999  14:12     4576  9CBD81AC
   IBM500        IBM500.___     11    12/02/1999  14:12     2304  14F6E36A
   IBM813        IBM813.___     11    12/02/1999  14:12     3072  6FC30F3A
   IBM819        IBM819.___     11    12/02/1999  14:12     2816  7FAABF61
   IBM829        IBM829.___     11    12/02/1999  14:12     3840  9E62075D
   IBM833        IBM833.___     11    12/02/1999  14:12     2272  424878C0
   IBM834        IBM834.___      8    12/02/1999  14:12   148704  C81D3534
   IBM835        IBM835.___      7    12/02/1999  14:12   125152  914F0E72
   IBM836        IBM836.___     11    12/02/1999  14:12     2272  37B66B24
   IBM837        IBM837.___      9    12/02/1999  14:12    84704  811F08FD
   IBM838        IBM838.___     11    12/02/1999  14:12     2272  07CF40C6
   IBM850        IBM850.___     11    12/02/1999  14:12     4320  711FAC6A
   IBM851        IBM851.___     11    12/02/1999  14:12     3840  6D400DD8
   IBM852        IBM852.___     11    12/02/1999  14:12     4608  A76091E3
   IBM855        IBM855.___     11    12/02/1999  14:12     4320  59F2A793
   IBM856        IBM856.___     11    12/02/1999  14:12     4064  448411D2
   IBM857        IBM857.___     11    12/02/1999  14:12     4352  1C9D6DB1
   IBM860        IBM860.___     11    12/02/1999  14:12     4320  6009A314
   IBM861        IBM861.___     11    12/02/1999  14:12     4064  4B58AAD3
   IBM862        IBM862.___     11    12/02/1999  14:12     4576  C2540C60
   IBM863        IBM863.___     11    12/02/1999  14:12     4096  471D68A9
   IBM864        IBM864.___     11    12/02/1999  14:12     4576  017C361E
   IBM865        IBM865.___     11    12/02/1999  14:12     4064  45E22FC9
   IBM866        IBM866.___     11    12/02/1999  14:12     4320  2DA50F82
   IBM868        IBM868.___     11    12/02/1999  14:12     4576  CEB47754
   IBM869        IBM869.___     11    12/02/1999  14:12     4320  3123486D
   IBM870        IBM870.___     11    12/02/1999  14:12     2560  66654884
   IBM871        IBM871.___     11    12/02/1999  14:12     2304  54DB4772
   IBM874        IBM874.___     11    12/02/1999  14:12     2784  98AEE14B
   IBM875        IBM875.___     11    12/02/1999  14:12     2528  0B7F3150
   IBM878        IBM878.___     11    12/02/1999  14:12     3328  8EEACD2D
   IBM891        IBM891.___     11    12/02/1999  14:12     3296  F14C1E09
   IBM895        IBM895.___     11    12/02/1999  14:12     2304  D8B7F493
   IBM896        IBM896.___     11    12/02/1999  14:12     2048  F849993B
   IBM897        IBM897.___     11    12/02/1999  14:12     3296  8DF97279
   IBM903        IBM903.___     11    12/02/1999  14:12     3296  D30CDC23
   IBM904        IBM904.___     11    12/02/1999  14:12     3040  C59759B4

   
                       FixPak Corrective Service levels and disk layouts  43


                   October 18, 2000 - Warp 3 FixPak XR_W043

   IBM907        IBM907.___     11    12/02/1999  14:12     3808  EF365739
   IBM909        IBM909.___     11    12/02/1999  14:12     3808  CDE491F3
   IBM910        IBM910.___     11    12/02/1999  14:12     3808  0623B68C
   IBM912        IBM912.___     11    12/02/1999  14:12     2560  3D919694
   IBM913        IBM913.___     11    12/02/1999  14:12     2560  AB1EE7D8
   IBM914        IBM914.___     11    12/02/1999  14:12     2560  2B0EC03E
   IBM915        IBM915.___     11    12/02/1999  14:12     2560  AA72BEC4
   IBM916        IBM916.___     11    12/02/1999  14:12     2560  D6D5399B
   IBM918        IBM918.___     11    12/02/1999  14:12     3040  EA1673D7
   IBM920        IBM920.___     11    12/02/1999  14:12     2560  C8191BF2
   IBM921        IBM921.___     11    12/02/1999  14:12     3040  0F0689F3
   IBM922        IBM922.___     11    12/02/1999  14:12     3040  71D4196C
   IBM930        IBM930.___      8    12/02/1999  14:12    94976  03764A56
   IBM931        IBM931.___      8    12/02/1999  14:12    94976  29B23D1C
   IBM933        IBM933.___      8    12/02/1999  14:12   149248  BF295A91
   IBM935        IBM935.___      8    12/02/1999  14:12    85248  54AA5F43
   IBM937        IBM937.___      7    12/02/1999  14:12   125696  9D8D65F3
   IBM939        IBM939.___      8    12/02/1999  14:12    94976  80873AC2
   IBM941        IBM941.___      8    12/02/1999  14:12    87264  0625D486
   IBM942        IBM942.___      8    12/02/1999  14:12    83712  E248EAFD
   IBM943        IBM943.___      8    12/02/1999  14:12    87808  28F19668
   IBM944        IBM944.___      8    12/02/1999  14:12   112896  A121A5E3
   IBM946        IBM946.___      8    12/02/1999  14:12    84736  7CE15C28
   IBM947        IBM947.___      7    12/02/1999  14:12   131808  F8506FE4
   IBM948        IBM948.___      7    12/02/1999  14:12   125696  F1BAF9FC
   IBM949        IBM949.___      8    12/02/1999  14:12   136448  8ECE1DF1
   IBM950        IBM950.___      6    12/02/1999  14:12   132352  69539457
   IBM952        IBM952.___      9    12/02/1999  14:12    89856  FC2DE730
   IBM953        IBM953.___     10    12/02/1999  14:12    83200  2E9BD4DE
   IBM954        IBM954.___      8    12/02/1999  14:12   140864  8321F0E0
   IBM955        IBM955.___      9    12/02/1999  14:12    89856  1FEF8CB2
   IBM964        IBM964.___      6    12/02/1999  14:12   174456  8767C8E3
   IBM970        IBM970.___      8    12/02/1999  14:12   169776  CD700829
   IBM971        IBM971.___      9    12/02/1999  14:12   124160  9D1C4C4C
   IFGDI2VM.DRV  IFGDI2VM.DR_    9    05/15/2000  16:23    93136  7268D00F
   IL.KBL        IL.KB_         11    12/02/1999  14:19     1232  21533791
   INSCFG32.DLL  INSCFG32.DL_   10    07/24/2000  19:15    31938  39D9CE7E
   INSPGM32.DLL  INSPGM32.DL_    9    07/24/2000  19:16    41504  DD5E5A69
   IS.KBL        IS.KB_         11    12/02/1999  14:19      940  552D9687
   IS458.KBL     IS458.KB_      11    12/02/1999  14:19      928  7634464C
   ISGDI2VM.DRV  ISGDI2VM.DR_    9    05/15/2000  16:07    92048  414AB307
   IT.KBL        IT.KB_         11    12/02/1999  14:19      876  6AF08922
   IT142.KBL     IT142.KB_      11    12/02/1999  14:19      854  FF50D3D2
   JP.KBL        JP.KB_         11    12/02/1999  14:19     6374  FA7C15A1
   KEYB.COM      KEYB.CO_       11    07/24/2000  22:49    11573  BD4A8679
   KEYBOARD.DCP  KEYBOARD.DC_   10    12/02/1999  14:21   315109  643C80C8
   KEYBOARD.DRV  KEYBOARD.DR_   11    07/19/1999  18:07     7568  DF5D49D9
   KR.KBL        KR.KB_         11    12/02/1999  14:19      724  0E4CB12A
   LA.KBL        LA.KB_         11    12/02/1999  14:19      916  BC6BAEDC
   LIBCM.DLL     LIBCM.DL_       4    11/22/1999  11:45   210916  98DAC320
   LIBCN.DLL     LIBCN.DL_       8    11/22/1999  11:45    57340  201E3106

   
                       FixPak Corrective Service levels and disk layouts  44


                   October 18, 2000 - Warp 3 FixPak XR_W043

   LIBCS.DLL     LIBCS.DL_       4    11/22/1999  11:45   192386  978DE493
   LIBUNI.DLL    LIBUNI.DL_      7    12/02/1999  14:22    81372  F5860058
   LINK386.EXE   LINK386.EX_     6    07/24/2000  22:59   154164  3609A24F
   LOCALE.DLL    LOCALE.DL_      6    12/02/1999  14:19   107901  50C0AEB5
   LT.KBL        LT.KB_         11    12/02/1999  14:19     1972  9614DF50
   LV.KBL        LV.KB_         11    12/02/1999  14:19     1404  07BED725
   LZEXPAND.DLL  LZEXPAND.DL_   10    07/19/1999  16:08    69040  482B530E
   MAIN.CPL      MAIN.CP_        7    07/19/1999  16:53   147680  C0023A80
   MAKETSF.EXE   MAKETSF.EX_     9    08/18/2000  15:38    43104  094AD175
   MAPTSF.CMD    MAPTSF.CM_     11    04/05/1999  09:56    16803  EA6B489C
   MCICDA.DRV    MCICDA.DR_     11    07/19/1999  17:11    13824  2E244338
   MCISEQ.DRV    MCISEQ.DR_     10    07/19/1999  17:11    25328  F76B8FE4
   MCIWAVE.DRV   MCIWAVE.DR_    10    07/19/1999  17:10    28160  8084128C
   MIDIMAP.DRV   MIDIMAP.DR_     9    07/19/1999  17:12    52800  4DCC5455
   MIGRATE.EXE   MIGRATE.EX_     6    07/24/2000  23:16   119434  C62DBE66
   MINXOBJ.DLL   MINXOBJ.DL_    10    07/25/2000  00:26    27423  BD6551E5
   MIRRORS.DLL   MIRRORS.DL_     2    03/12/1997  16:38   444744  4D9372B8
   MK.KBL        MK.KB_         11    12/02/1999  14:19     1302  1A6EFDD9
   MMSOUND.DRV   MMSOUND.DR_    11    07/19/1999  17:07     3456  97D7CBF0
   MMSYSTEM.DLL  MMSYSTEM.DL_    9    07/19/1999  17:06    61648  254ECC2F
   MMTASK.TSK    MMTASK.TS_     11    07/19/1999  17:06     1104  DCB8FD5B
   MOUSE.DRV     MOUSE.DR_      11    07/19/1999  18:10    10896  46184662
   MPLAYER.EXE   MPLAYER.EX_    10    07/19/1999  17:14    33312  C3711B4D
   MPU401.DRV    MPU401.DR_     11    07/19/1999  17:10     7088  BDC7982B
   MSADLIB.DRV   MSADLIB.DR_    11    07/19/1999  17:07    22048  82A78A36
   NL.KBL        NL.KB_         11    12/02/1999  14:19      954  87DF7272
   NO.KBL        NO.KB_         11    12/02/1999  14:19      920  54ED117D
   NOTEPAD.EXE   NOTEPAD.EX_    10    07/19/1999  16:17    32736  2788556F
   NPXEMLTR.DLL  NPXEMLTR.DL_   10    07/26/1999  20:55    21812  55B4EC1C
   NWIAPI.DLL    NWIAPI.DL_     11    07/24/2000  19:11     9149  5423C7DC
   OLECLI.DLL    OLECLI.DL_      9    07/19/1999  16:10    83456  30C78576
   OS2CHAR.DLL   OS2CHAR.DL_    11    08/26/1998  00:50      512  6828A757
   OS2DASD.DMD   OS2DASD.DM_    10    08/14/2000  18:07    40910  CED15CB1
   OS2DUMP       OS2DUMP.___    11    09/23/2000  17:55    14301  D86D377B
   OS2K386.EXE   OS2K386.EX_     8    07/19/1999  16:44    80306  BBCDD240
   OS2LDR.MSG    OS2LDR.MS_     11    09/23/2000  17:55     8737  DE8E117C
   OS2MM.DLL     OS2MM.DL_       3    12/07/1998  10:04   243830  D70109A0
   OS2UGL        OS2UGL.___     11    12/02/1999  14:12    15616  ACFC69CA
   OSO001.MSG    OSO001.MS_      8    12/04/1998  17:55   175769  8BFA1642
   OSO001H.MSG   OSO001H.MS_     7    12/04/1998  17:55   241212  303B0481
   PACKAGER.EXE  PACKAGER.EX_    9    07/19/1999  16:18    76464  B1B475D6
   PBRUSH.EXE    PBRUSH.EX_      7    07/19/1999  16:20   183360  DD6BEB29
   PDFSLA.EXE    PDFSLA.EX_     10    07/25/2000  00:00    18226  9FBE5971
   PDUMPSYS.EXE  PDUMPSYS.EX_   10    07/25/2000  00:58    34365  50AC8CDD
   PDUMPUSR.EXE  PDUMPUSR.EX_   10    07/25/2000  00:58    34363  2573EC10
   PL.KBL        PL.KB_         11    12/02/1999  14:19      980  F2F9E5B5
   PL457.KBL     PL457.KB_      11    12/02/1999  14:19      882  AECFDA03
   PMATM.DLL     PMATM.DL_       2    03/15/1999  18:36   224319  11C7F570
   PMBIND.DLL    PMBIND.DL_     10    07/24/2000  22:55    60162  7B6ABDDC
   PMCHKDSK.EXE  PMCHKDSK.EX_   10    07/24/2000  23:01    28183  FB650FB5
   PMCLIP.DLL    PMCLIP.DL_     10    07/24/2000  23:48    21315  D7548647

   
                       FixPak Corrective Service levels and disk layouts  45


                   October 18, 2000 - Warp 3 FixPak XR_W043

   PMCTLS.DLL    PMCTLS.DL_      2    07/24/2000  21:20   568344  74C0EE34
   PMDDE.DLL     PMDDE.DL_      10    07/24/2000  23:49    28170  9353EBCF
   PMDF.HLP      PMDF.HL_        8    01/09/1998  07:27    99751  BCE9E3DD
   PMDFMSG.DLL   PMDFMSG.DL_     9    07/28/1999  08:49    44436  3F51C356
   PMDRAG.DLL    PMDRAG.DL_     11    07/24/2000  21:12     1731  80203C5E
   PMGPI.DLL     PMGPI.DL_       3    07/24/2000  20:31   240974  54C0BFCD
   PMGRE.DLL     PMGRE.DL_      11    08/17/2000  10:45     2231  840E2F7E
   PMMLE.DLL     PMMLE.DL_      11    07/24/2000  21:19      673  11270A60
   PMPIC.DLL     PMPIC.DL_       9    07/24/2000  22:29    34870  42B0ACE8
   PMPIC.TDF     PMPIC.TD_      11    07/24/2000  22:29      400  1E15A7BD
   PMPRINT.QPR   PMPRINT.QP_    11    10/14/1998  21:04    12657  9EA7F7BD
   PMSDMRI.DLL   PMSDMRI.DL_    11    06/17/1998  16:54    13312  FD9863DF
   PMSEEK.EXE    PMSEEK.EX_     10    07/24/2000  23:08    31285  7E449FE0
   PMSHAPI.DLL   PMSHAPI.DL_    11    01/08/1998  16:40     4549  22E92C50
   PMSPL.DLL     PMSPL.DL_       3    08/18/2000  15:36   286151  4C625204
   PMSPL.TDF     PMSPL.TD_      11    08/18/2000  15:36     6930  8DC31673
   PMVDMP.DLL    PMVDMP.DL_      9    07/24/2000  22:13    42979  4B52953A
   PMVDMP.TDF    PMVDMP.TD_     11    07/24/2000  22:13     1786  6619142B
   PMVIOP.DLL    PMVIOP.DL_      8    07/24/2000  22:12    57740  C58F2974
   PMVIOP.TDF    PMVIOP.TD_     11    07/24/2000  22:12     2326  417547B6
   PMWIN.DLL     PMWIN.DL_      11    07/24/2000  20:51    11264  94A98194
   PMWP.DLL      PMWP.DL_        1    07/25/2000  00:21   961329  16E8396B
   PMWP.TDF      PMWP.TD_       11    07/25/2000  00:21    10855  7EDEFD46
   PMWPMRI.DLL   PMWPMRI.DL_     9    07/25/2000  00:07    46054  A5CE3E76
   PO.KBL        PO.KB_         11    12/02/1999  14:19      926  13EC7800
   PRINTMAN.EXE  PRINTMAN.EX_   10    07/19/1999  16:54    43248  4B7A98E5
   PROCDUMP.DOC  PROCDUMP.DO_   10    07/29/1998  18:07    63273  189C1459
   PROCDUMP.EXE  PROCDUMP.EX_    9    07/25/2000  00:57    47647  6B49E39E
   PROGMAN.EXE   PROGMAN.EX_     8    07/19/1999  16:51   115328  03CE0799
   PSSDMON.EXE   PSSDMON.EX_    10    07/24/2000  23:54    27117  F6D9EA78
   PSTAT.EXE     PSTAT.EX_      11    07/24/2000  23:08    11044  4B853F4F
   PVDAPI.DLL    PVDAPI.DL_     10    07/24/2000  23:53    20398  7801728F
   QUECALLS.DLL  QUECALLS.DL_   11    08/26/1998  01:30     1024  DB25D550
   RAS001.MSG    RAS001.MS_     11    01/09/1998  07:20    25739  5B41EDDD
   RASH.MSG      RASH.MS_       11    01/09/1998  07:20    11581  98CABDA3
   README.DBG    README.DB_     11    05/20/1999  13:28    22934  D76AEEF6
   RECOVER.COM   RECOVER.CO_     9    07/24/2000  23:09    48704  67FFD525
   REGEDIT.EXE   REGEDIT.EX_    10    06/18/1999  09:31    32336  2B8B6362
   REGEDIT.HLP   REGEDIT.HL_    10    07/19/1999  18:13    22682  E46C54AC
   RESTORE.EXE   RESTORE.EX_    10    07/24/2000  23:10    36080  5190E899
   REXX.DLL      REXX.DL_        4    04/05/1999  09:56   266031  2CB50B8E
   REXXAPI.DLL   REXXAPI.DL_    10    07/07/1998  16:42    40995  22013324
   REXXUTIL.DLL  REXXUTIL.DL_    7    08/23/2000  11:31    68119  4D4FB76B
   RO.KBL        RO.KB_         11    12/02/1999  14:19      944  AB98DE81
   RSPDSPI.EXE   RSPDSPI.EX_     7    07/24/2000  23:47    93192  37DBCD59
   RU.KBL        RU.KB_         11    12/02/1999  14:19     1144  48A696E0
   RU441.KBL     RU441.KB_      11    12/02/1999  14:19     1260  196F635B
   S8514.DRV     S8514.DR_       9    07/19/1999  17:43    89776  E601AA2F
   SD.KBL        SD.KB_         11    12/02/1999  14:19     1036  702BC72E
   SEAMLESS.DLL  SEAMLESS.DL_   10    07/24/2000  22:49    49125  5D53D83D
   SECUTIL.DLL   SECUTIL.DL_    10    07/24/2000  23:53    21468  0C32C5EC

   
                       FixPak Corrective Service levels and disk layouts  46


                   October 18, 2000 - Warp 3 FixPak XR_W043

   SEMAINT.EXE   SEMAINT.EX_     9    07/24/2000  23:19    66064  55003FE8
   SESAPI.DLL    SESAPI.DL_     10    07/24/2000  19:19    24155  8A8A57A9
   SESDB.DLL     SESDB.DL_      10    07/24/2000  23:52    23411  9FD0DFD5
   SESDMON.EXE   SESDMON.EX_    10    07/24/2000  23:54    26750  44D2EEC5
   SESMGR.DLL    SESMGR.DL_     11    08/26/1998  00:51     1536  E6962283
   SETBOOT.EXE   SETBOOT.EX_    10    07/24/2000  21:45    19760  DB57E92A
   SETUP.EXE     SETUP.EX_       6    07/19/1999  16:24   182448  38030DA4
   SF.KBL        SF.KB_         11    12/02/1999  14:19     1036  30F78793
   SHELL.DLL     SHELL.DL_      10    07/19/1999  16:50    32576  DA5FEBFA
   SIPANEL2.DLL  SIPANEL2.DL_   11    07/25/2000  00:31    53712  9B4BA2E8
   SK.KBL        SK.KB_         11    12/02/1999  14:19     1008  42A1D014
   SL.KBL        SL.KB_         11    12/02/1999  14:19      982  51F7B9B4
   SLDAPI.DLL    SLDAPI.DL_     10    07/24/2000  23:52    22441  2FEBB040
   SND.CPL       SND.CP_        11    07/19/1999  17:13     8192  E04657DB
   SNDBLST.DRV   SNDBLST.DR_    11    07/19/1999  17:08    13808  9F3A5354
   SNDBLST2.DRV  SNDBLST2.DR_   11    07/19/1999  17:09    14464  853178BB
   SOFTDRAW.DLL  SOFTDRAW.DL_    3    07/24/2000  19:23   416439  CAC786BD
   SOM.DLL       SOM.DL_         7    04/28/1997  18:07    92009  2CA2A023
   SOM.IR        SOM.IR_         5    03/12/1997  18:54   523185  402453DE
   SOMD.DLL      SOMD.DL_        3    03/12/1997  18:54   270638  CEA4A89C
   SOMD.MSG      SOMD.MS_       11    03/12/1997  18:54    15056  67D978FB
   SOMDD.EXE     SOMDD.EX_      10    03/12/1997  18:54    24928  3419526F
   SOMDSVR.EXE   SOMDSVR.EX_    10    03/12/1997  18:54    22800  6E2FC7B2
   SOMEM.DLL     SOMEM.DL_       9    03/12/1997  18:54    40132  8B31F245
   SOMIR.DLL     SOMIR.DL_       6    03/12/1997  18:54   110972  563D3A09
   SOMK.MSG      SOMK.MS_       11    03/12/1997  18:54     3724  C7CDF169
   SOMS.DLL      SOMS.DL_       10    03/12/1997  18:54    23074  719E33D8
   SOMTC.DLL     SOMTC.DL_       9    03/12/1997  18:54    35768  1B67EDCC
   SOMU.DLL      SOMU.DL_        7    03/12/1997  18:54    81652  DFFA1C69
   SOUND.DRV     SOUND.DR_      11    06/18/1999  09:31     3441  4F4AAE75
   SOUNDREC.EXE  SOUNDREC.EX_   10    07/19/1999  17:13    51305  04E55DB1
   SQ.KBL        SQ.KB_         11    12/02/1999  14:19      824  75B4805A
   SR.KBL        SR.KB_         11    12/02/1999  14:19     1222  8998A046
   STRACE.INF    STRACE.IN_      7    01/09/1998  07:31   153828  8838C9D0
   SV.KBL        SV.KB_         11    12/02/1999  14:19      946  80720FAB
   SYMB.PFM      SYM1.PF_       11    06/17/1998  14:49      679  46ACE0BD
   SYSDUMP.EXE   SYSDUMP.EX_    10    01/09/1998  07:29    16000  FE2B4A73
   SYSEDIT.EXE   SYSEDIT.EX_    11    07/19/1999  16:28    18896  3611E2AA
   SYSINST1.EXE  SYSINST1.EX_   11    01/09/1998  06:54     4224  58970725
   SYSINSTX.COM  SYSINSTX.CO_   10    09/23/2000  17:56    39472  E2FF1C21
   SYSLEVEL.EXE  SYSLEVEL.EX_    9    07/24/2000  22:45    43024  807A7408
   SYSLEVEL.FPK  SYSLEVEL.FP_   11    08/25/2000  15:27      165  311D3EF0
   SYSLEVEL.MSG  SYSLEVEL.MS_   11    07/24/2000  22:45     1445  FA956E54
   SYSLEVEL.SDS  SYSLEVEL.SD_   11    03/12/1997  18:54      265  735858E1
   SYSLEVEL.SEM  SYSLEVEL.SE_   11    03/12/1997  18:54      191  D0B7D94A
   SYSLEVEL.SIR  SYSLEVEL.SI_   11    03/12/1997  18:54      188  A7693C50
   SYSLEVEL.SRK  SYSLEVEL.SR_   11    03/12/1997  18:54      185  02859A09
   SYSLEVEL.SUT  SYSLEVEL.SUT   11    03/12/1997  18:54      177  A007547A
   SYSLOG.DLL    SYSLOG.DL_     11    07/24/2000  23:45     5681  2CE947FB
   SYSLOG.EXE    SYSLOG.EX_     11    07/24/2000  23:45     7204  8D3C8920
   SYSLOGPM.EXE  SYSLOGPM.EX_    9    07/24/2000  23:46    35478  E708EE18

   
                       FixPak Corrective Service levels and disk layouts  47


                   October 18, 2000 - Warp 3 FixPak XR_W043

   SYSMONO.FON   SYSMONO.FO_    10    06/17/1998  17:03    46255  88EACB2D
   SYSMONOI.FON  SYSMONOI.FO_   10    06/17/1998  17:03    46255  6803212B
   SYSSPLIT.CMD  SYSSPLIT.CM_   11    01/07/1998  17:08     3712  A32FABC8
   SYSTEM.DRV    SYSTEM.DR_     11    07/19/1999  16:56     2304  275E5C72
   TASKMAN.EXE   TASKMAN.EX_    11    07/19/1999  16:52     3744  E081632B
   TDFLST.CMD    TDFLST.CM_     11    04/05/1999  09:56    13564  61543592
   TEDIT.EXE     TEDIT.EX_      11    01/09/1998  04:02     9390  C58DDFE7
   TEXTCON1.EXE  TEXTCON1.EX_   10    11/23/1999  20:12    49011  5916B6E7
   TFFLST.CMD    TFFLST.CM_     11    04/05/1999  09:56     4638  12A615D0
   TH.KBL        TH.KB_         11    12/02/1999  14:19     1184  3D2E382C
   TH190.KBL     TH190.KB_      11    12/02/1999  14:19     1184  BBB3E598
   TIMER.DRV     TIMER.DR_      11    07/19/1999  17:07     4464  C7D0FA88
   TIMES.FON     TIMES.FO_       6    01/19/1998  13:36   257547  C00001C9
   TNR.OFM       TNR.OF_        11    02/12/1998  09:24     4882  65F1B2C9
   TNR.PFB       TNR.PF_         5    02/12/1998  09:24   119332  363246F5
   TNR.PFM       TN1.PF_        11    02/12/1998  09:24     1103  0CCC4E38
   TNRB.OFM      TNRB.OF_       11    02/12/1998  09:24     4898  551E8409
   TNRB.PFB      TNRB.PF_        5    02/12/1998  09:24   123083  E9834D17
   TNRB.PFM      TNR1.PF_       11    02/12/1998  09:24     1112  6035F3E3
   TNRBI.OFM     TNRBI.OF_      11    02/12/1998  09:24     4912  3A912F8F
   TNRBI.PFB     TNRBI.PF_       5    02/12/1998  09:24   134003  3B146D03
   TNRBI.PFM     TNRB1.PF_      11    02/12/1998  09:24     1118  8EDE75CB
   TNRI.OFM      TNRI.OF_       11    02/12/1998  09:24     4903  00B3E83C
   TNRI.PFB      TNRI.PF_        5    02/12/1998  09:24   131366  2C27E764
   TNRI.PFM      TNR2.PF_       11    02/12/1998  09:24     1114  27AE6580
   TOOLHELP.DLL  TOOLHELP.DL_   11    07/19/1999  16:14    14112  AB61F670
   TOUCH.DRV     TOUCH.DR_      11    07/19/1999  18:10    15760  044C9CF6
   TR.KBL        TR.KB_         11    12/02/1999  14:19      962  5DC99E17
   TR440.KBL     TR440.KB_      11    12/02/1999  14:19     1042  6D22006E
   TRACE.DOC     TRACE.DO_      10    04/05/1999  09:56    64057  95DDD0A2
   TRACE.EXE     TRACE.EX_       9    08/24/2000  09:42    35280  886E8B4D
   TRACEFMT.EXE  TRACEFMT.EX_    5    04/05/1999  20:44   155698  2B76B25F
   TRACEGET.EXE  TRACEGET.EX_   10    08/24/2000  09:42    22026  1126D207
   TRAPDUMP.EXE  TRAPDUMP.EX_   10    07/25/2000  00:58    16352  B0AFAABD
   TRAPLOG.EXE   TRAPLOG.EX_    10    01/09/1998  07:30    15056  5EE4C314
   TRC0007.TFF   TRC0007.TF_    11    07/24/2000  22:37     1041  11FA72A8
   TRC00C4.TFF   TRC00C4.TF_    11    07/24/2000  22:29      289  DB9FA422
   TRC00C6.TFF   TRC00C6.TF_    11    08/18/2000  15:36    11255  23E26239
   TRC0118.TFF   TRC0118.TF_    11    08/24/2000  09:41     2746  4B813DA6
   TRC0119.TFF   TRC0119.TF_    11    07/24/2000  21:43     3786  6E25B20C
   TRC012C.TFF   TRC012C.TF_    11    07/24/2000  22:13     3301  47BB5625
   TRC012D.TFF   TRC012D.TF_    11    07/24/2000  22:12     4739  7FC7B3D3
   TRC012E.TFF   TRC012E.TF_    11    07/25/2000  00:21    25717  5A554E19
   TRCUST.EXE    TRCUST.EX_      8    07/24/2000  19:28    98773  BBF8F3FC
   TRSPOOL.DOC   TRSPOOL.DO_     1    04/05/1999  09:56     6638  FC5E989C
   TRSPOOL.EXE   TRSPOOL.EX_    10    08/18/2000  15:38    27986  E0EF0896
   TW.KBL        TW.KB_         11    12/02/1999  14:19      780  23906445
   UA.KBL        UA.KB_         11    12/02/1999  14:19     1476  FDE0FA51
   UCDFS.DLL     UCDFS.DL_       8    01/08/1998  23:30    13264  8BD020DB
   UCONV.DLL     UCONV.DL_      10    12/02/1999  14:21    22819  AAC74ECC
   UCSTBL.LST    UCSTBL.LS_     11    11/22/1999  11:42     1789  78EC2A97

   
                       FixPak Corrective Service levels and disk layouts  48


                   October 18, 2000 - Warp 3 FixPak XR_W043

   UHPFS.DLL     UHPFS.DL_       7    08/24/2000  09:39   106000  DB3D3386
   UK.KBL        UK.KB_         11    12/02/1999  14:19      816  47EA3FBA
   UK168.KBL     UK168.KB_      11    12/02/1999  14:19      850  B43C6228
   ULS.REP       ULS.RE_        11    11/23/1999  13:33    19504  7FA91C1F
   ULSACT01.MSG  ULSACT01.MS_   11    11/23/1999  13:33      907  CCFEF741
   ULSCAU01.MSG  ULSCAU01.MS_   11    11/23/1999  13:33      899  5B2E152F
   ULSDET01.MSG  ULSDET01.MS_    7    11/23/1999  13:33      903  A0B1A1BE
   ULSERR01.MSG  ULSERR01.MS_   11    11/23/1999  13:33     1967  DB03FAC5
   UNICODE.SYS   UNICODE.SY_    11    12/02/1999  14:13    20014  71350E75
   UNIKBD.DLL    UNIKBD.DL_     10    12/02/1999  14:13    28515  58278529
   UNINSTAL.EXE  UNINSTAL.EX_    7    07/25/2000  00:51    94313  224D0BB8
   UNPACK2.EXE   UNPACK2.EX_     6    08/18/2000  15:39    79728  9265A7C7
   US.KBL        US.KB_         11    12/02/1999  14:19      774  8316962C
   USDV.KBL      USDV.KB_       11    12/02/1999  14:19      942  9E519962
   USDVL.KBL     USDVL.KB_      11    12/02/1999  14:19      924  040B0F6A
   USDVR.KBL     USDVR.KB_      11    12/02/1999  14:19      942  2624513F
   USER.EXE      USER.EX_        4    07/19/1999  17:02   281008  7AFB68FB
   USINTER.KBL   USINTER.KB_    11    12/02/1999  14:19     1032  5FE88FD9
   VBIOS.SYS     VBIOS.SY_      11    07/24/2000  23:23     8816  DBA67F95
   VCMOS.SYS     VCMOS.SY_      11    07/24/2000  23:23     2272  85C719BE
   VDMA.SYS      VDMAPS2.SY_    11    07/24/2000  23:25    14329  018914A3
   VDMA.SYS      VDMAAT.SY_     11    07/24/2000  23:24    11465  7C819F8B
   VDPMI.SYS     VDPMI.SY_      11    07/24/2000  23:27    22385  7586B6FD
   VDPX.SYS      VDPX.SY_       10    07/24/2000  23:02    25857  FB2744C4
   VER.DLL       VER.DL_         4    07/19/1999  16:13     9008  5353A52A
   VIOTBL.DCP    VIOTBL.DC_     10    12/02/1999  14:20   225355  406F489E
   VIOTBL.ISO    VIOTBL.IS_      9    12/02/1999  14:21   230105  2FE2121C
   VMAN.DLL      VMAN.DL_        9    08/06/2000  12:13    61017  EEF32ED5
   VMANWIN.SYS   VMANWIN.SY_    11    07/10/2000  14:07     3040  C2F3E282
   VW32S.SYS     VW32S.SY_       9    07/24/2000  21:47    18289  DA76264F
   VWIN.SYS      VWIN.SY_       10    07/24/2000  23:41    26912  1EF1992A
   WIN.COM       WIN.CO_        10    07/19/1999  17:03    44651  91A9CCC5
   WINFILE.EXE   WINFILE.EX_     7    07/19/1999  16:52   146960  A5D456E1
   WINOS2.COM    WINOS2.CO_     10    07/19/1999  17:03    16592  34A9D3F5
   WINSCLIP.DLL  WINSCLIP.DL_   11    07/19/1999  16:49    14848  063E0199
   WINSDDE.DLL   WINSDDE.DL_    11    07/19/1999  16:49    18432  A4D90F73
   WINSHELD.EXE  WINSHELD.EX_   11    07/19/1999  16:49    22016  50F1265D
   WINSMSG.DLL   WINSMSG.DL_    11    07/19/1999  16:49    28441  331BB9D3
   WINVER.EXE    WINVER.EX_     11    07/19/1999  16:27     3904  A3F20381
   WPCMPNP.DLL   WPCMPNP.DL_     7    01/09/1998  06:23    73433  C85C4DFF
   WPCONFIG.DLL  WPCONFIG.DL_    1    07/26/1999  22:10   220139  9DB983B4
   WPCONMRI.DLL  WPCONMRI.DL_   10    01/09/1998  06:42    16777  C0C8F0AC
   WPHELP.HLP    WPHELP.HL_      2    07/24/2000  23:36   713080  B8D0EBE2
   WPPRINT.DLL   WPPRINT.DL_     3    07/25/2000  00:25   365740  2DDCFA1D
   WPPRINT.HLP   WPPRINT.HL_     8    01/09/1998  06:13    71408  27006DF2
   WPPRTMRI.DLL  WPPRTMRI.DL_    9    01/09/1998  06:13    54486  EBE95633
   WRITE.EXE     WRITE.EX_       5    07/19/1999  16:33   244976  C99E812D
   WSPDBF.DRV    WSPDBF.DR_      8    07/19/1999  17:38   108512  E4E01A2F
   WSPDSBF.DRV   WSPDSBF.DR_     8    07/19/1999  17:39   109568  2B67AE15
   WSPDSF.DRV    WSPDSF.DR_      8    07/19/1999  17:38   106032  7F2A0817
   WSPDSSF.DRV   WSPDSSF.DR_     8    07/19/1999  17:39   107088  205D36A3

   
                       FixPak Corrective Service levels and disk layouts  49


                   October 18, 2000 - Warp 3 FixPak XR_W043

   XCOPY.EXE     XCOPY.EX_       9    07/24/2000  23:37    51616  D97DE90A
   XDFH.MSG      XDFH.MS_        9    07/24/2000  22:44     1045  4FE7C3D5
   XPG00420.TBL  XPG00420.TB_   11    11/22/1999  12:17    27264  48667C1E
   XPG00864.TBL  XPG00864.TB_   11    11/22/1999  12:17    27264  76725C6C

   ************************************************************************
   Product location on CSD:  A:\FIX\OS2.2
   Product name:  "IBM OS/2 Base Operating System"
   Standard Edition  3.01
   Fixpak name:   XR_W043_   (Country = Generic)
   Pre-requisite CSD Level:  XR_3005_
   System Id:  1000
   Component Id:  562274700
   Archive is ON for this product.
   ________________________________________________________________________

   Default directories:

           ..\..\
           ..\*
           ..\..\VT
           ..\..\VT\*
           ..\..\PSFONTS
           ..\..\PSFONTS\*
           ..\..\LANGUAGE
           ..\..\LANGUAGE\*

   Files contained in Fixpak for product:

   Filename      Name on CSD   Disk#  Date        Time   Size     Checksum
   ------------  ------------  -----  ----------  -----  -------  --------
   BVHVGA.DLL    BVHVGA.DL_     13    02/17/1998  15:37    31847  3C3497E0
   DF_DEB.EXE    DF_DEB.EX_     13    07/24/2000  21:11   136061  1190A466
   DF_RET.EXE    DF_RET.EX_     13    07/24/2000  21:11   136029  9A2915DE
   DOSCALL1.DLL  DOSCALL1.DL_   11    07/24/2000  19:24   125480  45DF7BAD
   DOSCALL1.TDF  DOSCALL1.TD_   13    07/24/2000  19:24     5426  EE8777BD
   DOSKRNL       DOSKRNL.___    13    07/24/2000  19:21    30509  0DF905BB
   GETMONID.CMD  GETMONID.CM_   13    03/15/1999  13:49     2426  47BB3FE5
   INSTALL.EXE   INSTALL.EX_    12    07/24/2000  20:57   302747  9C58053F
   KBDBASE.SYS   KBDBASE.SY_    13    07/19/2000  12:30    25021  B4C8D21E
   KERNEL.SDF    KERNEL.SD_     13    07/24/2000  21:13    55657  D6B3FFE8
   KERNELD.SDF   KERNELD.SD_    13    07/24/2000  21:14    55735  053970B5
   KRNLBDEV.TDF  KRNLBDEV.TD_   13    09/25/2000  13:40     3314  850AEBB5
   KRNLBFS.TDF   KRNLBFS.TD_    13    09/25/2000  13:40     4572  CB03AE0C
   KRNLBLDR.TDF  KRNLBLDR.TD_   13    09/25/2000  13:40     5497  F500F82E
   KRNLBPG.TDF   KRNLBPG.TD_    13    09/25/2000  13:40     3203  C0FC9F8E
   KRNLBSEL.TDF  KRNLBSEL.TD_   13    09/25/2000  13:40     2369  09BD37A2
   KRNLBSEM.TDF  KRNLBSEM.TD_   13    09/25/2000  13:40     1353  67689620
   KRNLBSM.TDF   KRNLBSM.TD_    13    09/25/2000  13:40     1321  93064B4B
   KRNLBTK.TDF   KRNLBTK.TD_    13    09/25/2000  13:40    14180  F9931D8F
   KRNLBTOM.TDF  KRNLBTOM.TD_   13    09/25/2000  13:40      925  0221FEC6

   
                       FixPak Corrective Service levels and disk layouts  50


                   October 18, 2000 - Warp 3 FixPak XR_W043

   KRNLBVDM.TDF  KRNLBVDM.TD_   13    09/25/2000  13:40    17560  7F99BF47
   KRNLBVM.TDF   KRNLBVM.TD_    13    09/25/2000  13:40     5293  5F083CD3
   KRNLDDEV.TDF  KRNLDDEV.TD_   13    09/25/2000  13:39     3314  8FA379A9
   KRNLDFS.TDF   KRNLDFS.TD_    13    09/25/2000  13:39     4538  1488A588
   KRNLDLDR.TDF  KRNLDLDR.TD_   13    09/25/2000  13:39     5500  B05FC61C
   KRNLDPG.TDF   KRNLDPG.TD_    13    09/25/2000  13:39     3284  28174535
   KRNLDSEL.TDF  KRNLDSEL.TD_   13    09/25/2000  13:39     2425  96282968
   KRNLDSEM.TDF  KRNLDSEM.TD_   13    09/25/2000  13:39     1493  72E5546A
   KRNLDSM.TDF   KRNLDSM.TD_    13    09/25/2000  13:39     1321  0AF11429
   KRNLDTK.TDF   KRNLDTK.TD_    13    09/25/2000  13:39    14286  F5479021
   KRNLDTOM.TDF  KRNLDTOM.TD_   13    09/25/2000  13:39      953  5339EA8A
   KRNLDVDM.TDF  KRNLDVDM.TD_   13    09/25/2000  13:39    17635  72A5B58E
   KRNLDVM.TDF   KRNLDVM.TD_    13    09/25/2000  13:39     5405  429C0D13
   KRNLRDEV.TDF  KRNLRDEV.TD_   13    09/25/2000  13:37     3314  65DBD521
   KRNLRFS.TDF   KRNLRFS.TD_    13    09/25/2000  13:37     4597  4D3A8E1F
   KRNLRLDR.TDF  KRNLRLDR.TD_   13    09/25/2000  13:37     5472  26949C21
   KRNLRPG.TDF   KRNLRPG.TD_    13    09/25/2000  13:38     3203  38A6A180
   KRNLRSEL.TDF  KRNLRSEL.TD_   13    09/25/2000  13:38     2369  3BFFF7B3
   KRNLRSEM.TDF  KRNLRSEM.TD_   13    09/25/2000  13:38     1353  92536947
   KRNLRSM.TDF   KRNLRSM.TD_    13    09/25/2000  13:38     1321  FCF4EF39
   KRNLRTK.TDF   KRNLRTK.TD_    13    09/25/2000  13:38    14096  47A303D2
   KRNLRTOM.TDF  KRNLRTOM.TD_   13    09/25/2000  13:38      897  E628FE9F
   KRNLRVDM.TDF  KRNLRVDM.TD_   13    09/25/2000  13:37    17242  5C2B66A0
   KRNLRVM.TDF   KRNLRVM.TD_    13    09/25/2000  13:38     5293  E5D867BB
   MONCALLS.TDF  MONCALLS.TD_   13    07/24/2000  19:22     1139  6AB63A8C
   OS2CHAR.TDF   OS2CHAR.TD_    13    07/24/2000  19:24    13889  148319BB
   OS2KRNL       OS2KRNL.___    11    09/25/2000  13:38   634314  1C5B6FAF
   OS2KRNL.TDF   OS2KRNL.TD_    13    09/25/2000  13:37    16609  6D399A29
   OS2KRNLB.TDF  OS2KRNLB.TD_   13    09/25/2000  13:40    16609  7B7DE4C6
   OS2KRNLD.TDF  OS2KRNLD.TD_   13    09/25/2000  13:39    16609  0DCE8081
   OS2LDR        OS2LDR.___     13    09/23/2000  17:54    33280  9934916D
   PMDF.EXE      PMDF.EX_       13    07/24/2000  21:13   260024  C7C82016
   PMDFINST.CMD  PMDFINST.CM_   13    01/07/1998  17:10    18501  61C6F001
   PMGPI.TDF     PMGPI.TD_      13    07/24/2000  20:19    12338  74FB2856
   PMGRE.TDF     PMGRE.TD_      13    07/24/2000  21:12     1062  512B0C38
   PMMERGE.DLL   PMMERGE.DL_    12    07/24/2000  21:12  1335998  DA95F37A
   PMSHAPI.TDF   PMSHAPI.TD_    13    07/24/2000  21:12     6751  0D242ED0
   PMWIN.TDF     PMWIN.TD_      13    07/24/2000  21:12    13570  CBB0C971
   PMWIN32.SDF   PMWIN32.SD_    13    07/24/2000  21:14    33388  BEE59D2E
   QUECALLS.TDF  QUECALLS.TD_   13    07/24/2000  19:24     1319  B7B21859
   RSPINST.EXE   RSPINST.EX_    13    07/24/2000  21:03   289706  23A17478
   RUPINST2.EXE  RUPINST2.EX_   12    07/24/2000  21:00   173120  21E0BCB6
   RXVIDCFG.DLL  RXVIDCFG.DL_   13    04/07/1999  16:04    14741  4698736B
   SESDD32.SYS   SESDD32.SY_    13    07/24/2000  20:47   118833  3F07B28D
   SESMGR.TDF    SESMGR.TD_     13    07/24/2000  19:24     1877  8A6DE498
   SHELL.SDF     SHELL.SD_      13    07/24/2000  21:14    20418  CB4388DE
   SOMCT.DLL     SOMCT.DL_      13    04/28/1997  18:06    42841  A6FF6813
   SOMSEC.DLL    SOMSEC.DL_     11    04/28/1997  18:06    33214  1A34710E
   SOMUC.DLL     SOMUC.DL_      13    04/28/1997  18:06    86276  BA4B46D0
   STRACE.EXE    STRACE.EX_     13    07/24/2000  21:15    41010  6A6A85F6
   SYSINST2.EXE  SYSINST2.EX_   13    07/24/2000  20:59   171808  5FC0B0A7

   
                       FixPak Corrective Service levels and disk layouts  51


                   October 18, 2000 - Warp 3 FixPak XR_W043

   SYSLEVEL.SCT  SYSLEVEL.SC_   13    06/16/1998  17:42      187  9FD92CA3
   SYSLEVEL.SUC  SYSLEVEL.SUC   13    06/16/1998  17:42      191  665CE147
   TRACE.HLP     TRACE.HL_      13    04/05/1999  18:12    29376  DF1AC854
   TRACEFMT.ICO  TRACEFMT.IC_   13    03/12/1997  17:08     2692  510E56CA
   TRC0000.TFF   TRC0000.TF_    13    01/25/1999  10:24      189  78DB2563
   TRC0003.TFF   TRC0003.TF_    13    01/25/1999  10:24     1503  0DDD868D
   TRC0004.TFF   TRC0004.TF_    13    09/25/2000  11:01     4754  EDA2826B
   TRC0005.TFF   TRC0005.TF_    13    09/25/2000  13:40    38800  6E9E4F39
   TRC0006.TFF   TRC0006.TF_    13    01/25/1999  09:53    12356  8DD5674E
   TRC0010.TFF   TRC0010.TF_    13    07/24/2000  19:24    13359  60C2A17F
   TRC0016.TFF   TRC0016.TF_    13    07/24/2000  19:24     1719  29E34E3E
   TRC0017.TFF   TRC0017.TF_    13    07/24/2000  19:24     5561  E8B3BD71
   TRC0018.TFF   TRC0018.TF_    13    07/24/2000  19:24    39488  29C61366
   TRC00C0.TFF   TRC00C0.TF_    13    07/24/2000  21:12    16022  20415253
   TRC00C2.TFF   TRC00C2.TF_    13    07/24/2000  21:12    34340  3A188B88
   TRC00C3.TFF   TRC00C3.TF_    13    07/24/2000  21:12     3984  F96F4AC7
   TRC00C5.TFF   TRC00C5.TF_    13    07/24/2000  20:19    32994  870F1018
   TRC0100.TFF   TRC0100.TF_    13    09/25/2000  13:40     5475  04A7A7D9
   TRC0101.TFF   TRC0101.TF_    13    09/25/2000  13:40     7557  1122EE24
   TRC0102.TFF   TRC0102.TF_    13    09/25/2000  13:40    34804  B4DE818E
   TRC0103.TFF   TRC0103.TF_    13    09/25/2000  13:40     9891  254E2B21
   TRC0104.TFF   TRC0104.TF_    13    09/25/2000  13:40     5135  C63FDFBD
   TRC0105.TFF   TRC0105.TF_    13    09/25/2000  13:40    27788  E221FE02
   TRC0106.TFF   TRC0106.TF_    13    09/25/2000  13:40     1835  59FAB074
   TRC0107.TFF   TRC0107.TF_    12    09/25/2000  13:40     3732  0307A335
   TRC0108.TFF   TRC0108.TF_    11    09/25/2000  13:40     9082  33D53052
   TRC0109.TFF   TRC0109.TF_    13    09/25/2000  13:40     1713  1C40CCB5
   TRC010A.TFF   TRC010A.TF_    13    09/25/2000  13:40     1029  FDEB4F4F
   TRCFORMT.DLL  TRCFORMT.DL_   13    10/14/1998  20:27    26630  1C6837BB
   VCFGCID.CMD   VCFGCID.CM_    13    03/15/1999  13:49    13187  E79BE969
   VMOUSE.SYS    VMOUSE.SY_     13    07/24/2000  19:57    17280  C234CFE8
   VPIC.SYS      VPIC.SY_       13    07/24/2000  19:58     9942  91BA55C2
   VPICPARM.SYS  VPICPARM.SY_   13    07/24/2000  19:58      736  A3AC54AA
   VTIMER.SYS    VTIMER.SY_     13    07/24/2000  19:59     9936  B627CF2E
   VXGA.SYS      VXGA.SY_       12    02/17/1998  15:37    24771  0727963F

   ************************************************************************
   Product location on CSD:  A:\FIX\OS2.3
   Product name:  "IBM OS/2 Base Operating System"
   Standard Edition  3.02
   Fixpak name:   XR_W043_   (Country = Generic)
   Pre-requisite CSD Level:  XR_3006_
   System Id:  1000
   Component Id:  5639A5500
   Archive is ON for this product.
   ________________________________________________________________________

   Default directories:

           ..\..\
           ..\*

   
                       FixPak Corrective Service levels and disk layouts  52


                   October 18, 2000 - Warp 3 FixPak XR_W043

           ..\..\VT
           ..\..\VT\*
           ..\..\PSFONTS
           ..\..\PSFONTS\*
           ..\..\LANGUAGE
           ..\..\LANGUAGE\*

   Files contained in Fixpak for product:

   Filename      Name on CSD   Disk#  Date        Time   Size     Checksum
   ------------  ------------  -----  ----------  -----  -------  --------
   ALR.PSD       ALR.PS_        16    07/24/2000  19:16    18432  E5F17A7D
   CAVERUN.PSD   CAVERUN.PS_    16    07/24/2000  19:17    29184  8E5B1630
   DF_DEB.EXE    DF_DEB.EX_     16    07/25/2000  00:54   144949  12423600
   DF_RET.EXE    DF_RET.EX_     16    07/25/2000  00:53   144917  6CEE25DF
   DOSCALL1.DLL  DOSCALL1.DL_   15    07/24/2000  21:56   137960  10EF703F
   DOSCALL1.SYM  DOSCALL1.SY_   16    07/24/2000  21:56    42740  8C464683
   DOSCALL1.TDF  DOSCALL1.TD_   16    07/24/2000  21:56     5534  A4588FDF
   DOSKRNL       DOSKRNL.___    16    07/24/2000  21:31    30525  C9052EFD
   INSTALL.EXE   INSTALL.EX_    14    07/25/2000  00:37   304595  D6A93019
   KBDBASE.SYS   KBDBASE.SY_    16    07/19/2000  12:34    24989  DD68564A
   KERNEL.SDF    KERNEL.SD_     16    07/25/2000  00:57    57011  6C2C0512
   KERNELD.SDF   KERNELD.SD_    16    07/25/2000  00:57    57136  056B67DC
   KRNLBDEV.TDF  KRNLBDEV.TD_   16    09/25/2000  13:40     4279  4A3DE8BD
   KRNLBFS.TDF   KRNLBFS.TD_    16    09/25/2000  13:40     4899  46304E8F
   KRNLBLDR.TDF  KRNLBLDR.TD_   16    09/25/2000  13:40     5609  865BDB7F
   KRNLBPG.TDF   KRNLBPG.TD_    16    09/25/2000  13:40     3427  6AD4B4BB
   KRNLBSEL.TDF  KRNLBSEL.TD_   16    09/25/2000  13:40     2755  B32DA9CC
   KRNLBSEM.TDF  KRNLBSEM.TD_   16    09/25/2000  13:40     1764  EB8C892C
   KRNLBSM.TDF   KRNLBSM.TD_    16    09/25/2000  13:40     1321  36FCF4D7
   KRNLBTK.TDF   KRNLBTK.TD_    16    09/25/2000  13:40    15892  E4C075FD
   KRNLBTOM.TDF  KRNLBTOM.TD_   16    09/25/2000  13:40     1009  9BFC4126
   KRNLBVDM.TDF  KRNLBVDM.TD_   16    09/25/2000  13:40    17831  4FD6D8B1
   KRNLBVM.TDF   KRNLBVM.TD_    16    09/25/2000  13:40     5321  BA713337
   KRNLDDEV.TDF  KRNLDDEV.TD_   16    09/25/2000  13:37     4279  0F9ABCB2
   KRNLDFS.TDF   KRNLDFS.TD_    16    09/25/2000  13:37     4865  D0AC8946
   KRNLDLDR.TDF  KRNLDLDR.TD_   16    09/25/2000  13:38     5637  A802D470
   KRNLDPG.TDF   KRNLDPG.TD_    16    09/25/2000  13:38     3508  12CA5953
   KRNLDSEL.TDF  KRNLDSEL.TD_   16    09/25/2000  13:38     2867  BD9877B6
   KRNLDSEM.TDF  KRNLDSEM.TD_   16    09/25/2000  13:38     1932  BC04424E
   KRNLDSM.TDF   KRNLDSM.TD_    16    09/25/2000  13:38     1321  2BAED117
   KRNLDTK.TDF   KRNLDTK.TD_    16    09/25/2000  13:38    16023  2F86D4B3
   KRNLDTOM.TDF  KRNLDTOM.TD_   16    09/25/2000  13:38     1037  2F5B8648
   KRNLDVDM.TDF  KRNLDVDM.TD_   16    09/25/2000  13:38    17881  2A62A101
   KRNLDVM.TDF   KRNLDVM.TD_    16    09/25/2000  13:38     5433  5F8C7812
   KRNLRDEV.TDF  KRNLRDEV.TD_   16    09/25/2000  13:39     4279  616E3EC6
   KRNLRFS.TDF   KRNLRFS.TD_    16    09/25/2000  13:39     4899  4B693890
   KRNLRLDR.TDF  KRNLRLDR.TD_   16    09/25/2000  13:39     5609  BA5CF59D
   KRNLRPG.TDF   KRNLRPG.TD_    16    09/25/2000  13:39     3427  239EBD53
   KRNLRSEL.TDF  KRNLRSEL.TD_   16    09/25/2000  13:39     2755  B70AE9C1
   KRNLRSEM.TDF  KRNLRSEM.TD_   16    09/25/2000  13:39     1764  315FD8D3

   
                       FixPak Corrective Service levels and disk layouts  53


                   October 18, 2000 - Warp 3 FixPak XR_W043

   KRNLRSM.TDF   KRNLRSM.TD_    16    09/25/2000  13:39     1321  5158EBAC
   KRNLRTK.TDF   KRNLRTK.TD_    16    09/25/2000  13:39    15808  18D65227
   KRNLRTOM.TDF  KRNLRTOM.TD_   16    09/25/2000  13:39      981  BCC6A059
   KRNLRVDM.TDF  KRNLRVDM.TD_   16    09/25/2000  13:39    17513  1896CC3E
   KRNLRVM.TDF   KRNLRVM.TD_    16    09/25/2000  13:39     5321  1E05F612
   MONCALLS.TDF  MONCALLS.TD_   16    07/24/2000  21:51     1139  6AB4753C
   OS2APIC.PSD   OS2APIC.PS_    16    07/24/2000  19:18    31232  06DFE794
   OS2CHAR.TDF   OS2CHAR.TD_    16    07/24/2000  21:56    13889  89827E0A
   OS2KRNL       OS2KRNL.___    15    09/25/2000  13:39   729234  BDC9CDE4
   OS2KRNL.TDF   OS2KRNL.TD_    16    09/25/2000  13:39    16837  05503D4D
   OS2KRNLB.SYM  OS2KRNLB.SY_   15    09/25/2000  13:40   192612  0BD959BA
   OS2KRNLB.TDF  OS2KRNLB.TD_   16    09/25/2000  13:40    16837  98918FF7
   OS2KRNLD.SYM  OS2KRNLD.SY_   15    09/25/2000  13:37   195604  B1CC4FB8
   OS2KRNLD.TDF  OS2KRNLD.TD_   16    09/25/2000  13:37    16867  ABA5ADB7
   OS2KRNLR.SYM  OS2KRNLR.SY_   13    09/25/2000  13:39   173652  89FEE965
   OS2LDR        OS2LDR.___     16    09/23/2000  17:54    35000  3A155991
   PMCTLS.SYM    PMCTLS.SY_     15    07/24/2000  21:20    43508  05FFEC59
   PMDD.SYM      PMDD.SY_       16    07/24/2000  23:06     2740  39C734BF
   PMDDE.SYM     PMDDE.SY_      16    07/24/2000  23:49     2500  D2133706
   PMDF.EXE      PMDF.EX_       15    07/25/2000  00:56   260028  0DE435BE
   PMDRAG.SYM    PMDRAG.SY_     16    07/24/2000  21:12       36  FC6F4BE7
   PMGPI.SYM     PMGPI.SY_      16    07/24/2000  20:32    46708  A60E75F4
   PMGPI.TDF     PMGPI.TD_      16    07/24/2000  20:32    12338  4A7B283F
   PMGRE.TDF     PMGRE.TD_      16    08/18/2000  07:41     1062  3CAC6ADE
   PMMERGE.DLL   PMMERGE.DL_    14    08/18/2000  07:42  1336372  3CB34385
   PMMERGE.SYM   PMMERGE.SY_    16    08/18/2000  07:41    92564  72FC458D
   PMMLE.SYM     PMMLE.SY_      16    07/24/2000  21:19       36  CC21FB55
   PMPIC.SYM     PMPIC.SY_      16    07/24/2000  22:29     8436  C698A770
   PMPRINT.SYM   PMPRINT.SY_    16    08/18/2000  15:35     1636  1A207904
   PMSHAPI.TDF   PMSHAPI.TD_    14    08/18/2000  07:41     6751  6AB9DC9C
   PMSHELL.SYM   PMSHELL.SY_    16    07/25/2000  00:06      500  BDC92418
   PMSPL.SYM     PMSPL.SY_      16    08/18/2000  15:36    32436  4C9B0A64
   PMSPOOL.SYM   PMSPOOL.SY_    16    07/26/1999  19:33      404  BAFD842C
   PMVDMP.SYM    PMVDMP.SY_     16    07/24/2000  22:13     5268  743EDF3C
   PMVIOP.SYM    PMVIOP.SY_     16    07/24/2000  22:12     6404  28F623A5
   PMWIN.TDF     PMWIN.TD_      16    08/18/2000  07:41    13570  202012E2
   PMWIN32.SDF   PMWIN32.SD_    16    07/25/2000  00:57    33419  16C2F123
   PMWP.SYM      PMWP.SY_       16    07/25/2000  00:21    95972  80AE9164
   PROLIANT.PSD  PROLIANT.PS_   16    07/24/2000  19:18    18944  9B185EE4
   QUECALLS.TDF  QUECALLS.TD_   16    07/24/2000  21:56     1319  48BC83B3
   RSPDDI.EXE    RSPDDI.EX_     16    07/24/2000  22:57    22073  25D3A600
   RSPINST.EXE   RSPINST.EX_    15    07/25/2000  00:46   290825  3A06E599
   RUPINST2.EXE  RUPINST2.EX_   14    07/25/2000  00:41   172096  9E0129FD
   SESDD32.SYS   SESDD32.SY_    16    09/25/2000  10:48   118833  EC906600
   SESMGR.TDF    SESMGR.TD_     16    07/24/2000  21:56     1877  5EE631E5
   SHELL.SDF     SHELL.SD_      16    07/25/2000  00:57    20425  B0547CB6
   STRACE.EXE    STRACE.EX_     16    07/25/2000  00:58    41010  783585F5
   SYSINST2.EXE  SYSINST2.EX_   16    07/25/2000  00:41   170784  00D74AB5
   SYSLOGPM.EXE  SYSLOGPM.EX_   16    07/24/2000  23:46    35478  E708EE18
   TRACE.HLP     TRACE.HL_      16    04/05/1999  20:44    29376  DFB82054
   TRC0000.TFF   TRC0000.TF_    16    08/11/1998  19:53      189  CEDB268C

   
                       FixPak Corrective Service levels and disk layouts  54


                   October 18, 2000 - Warp 3 FixPak XR_W043

   TRC0003.TFF   TRC0003.TF_    16    08/11/1998  19:53     1503  B3358691
   TRC0004.TFF   TRC0004.TF_    16    09/25/2000  10:42     4754  FA4D826B
   TRC0005.TFF   TRC0005.TF_    16    09/25/2000  13:40    39307  E9EF5D99
   TRC0006.TFF   TRC0006.TF_    16    08/11/1998  18:51    12356  AF80674E
   TRC0010.TFF   TRC0010.TF_    16    07/24/2000  21:56    13647  C63E083D
   TRC0016.TFF   TRC0016.TF_    16    07/24/2000  21:56     1719  7FE34E65
   TRC0017.TFF   TRC0017.TF_    16    07/24/2000  21:56     5561  3EB3BD99
   TRC0018.TFF   TRC0018.TF_    16    07/24/2000  21:56    39488  9F261368
   TRC00C0.TFF   TRC00C0.TF_    16    08/18/2000  07:41    16022  20131D13
   TRC00C2.TFF   TRC00C2.TF_    16    08/18/2000  07:41    34340  73708B82
   TRC00C3.TFF   TRC00C3.TF_    16    08/18/2000  07:41     3984  8EEF4A6B
   TRC00C5.TFF   TRC00C5.TF_    16    07/24/2000  20:32    32994  87037AD8
   TRC0100.TFF   TRC0100.TF_    13    09/25/2000  13:40     7355  BE5C1C68
   TRC0101.TFF   TRC0101.TF_    16    09/25/2000  13:40     8178  79210C9E
   TRC0102.TFF   TRC0102.TF_    16    09/25/2000  13:40    35318  620B6A64
   TRC0103.TFF   TRC0103.TF_    16    09/25/2000  13:40    10111  3D6CAA6A
   TRC0104.TFF   TRC0104.TF_    16    09/25/2000  13:40     5574  8FC9972B
   TRC0105.TFF   TRC0105.TF_    16    09/25/2000  13:40    31306  2AB9C9AE
   TRC0106.TFF   TRC0106.TF_    16    09/25/2000  13:40     1835  B1FAB071
   TRC0107.TFF   TRC0107.TF_    16    09/25/2000  13:40     4462  152E7E07
   TRC0108.TFF   TRC0108.TF_    16    09/25/2000  13:40     9131  F3DB24C9
   TRC0109.TFF   TRC0109.TF_    16    09/25/2000  13:40     2483  7817B7CF
   TRC010A.TFF   TRC010A.TF_    16    09/25/2000  13:40     1175  86E593DF
   TRCFORMT.DLL  TRCFORMT.DL_   16    10/14/1998  22:11    26630  1C838DBB
   TRICRD.PSD    TRICRD.PS_     16    07/24/2000  19:18     4608  56023051
   V1_EBI2.PSD   V1_EBI2.PS_    14    07/24/2000  19:17    19456  0D290E76
   VIPERMP.PSD   VIPERMP.PS_    16    07/24/2000  19:19     6656  6FB5B2A8
   VMOUSE.SYS    VMOUSE.SY_     16    07/24/2000  23:32    17280  230A9DB6
   VPIC.SYS      VPIC.SY_       16    07/24/2000  23:33     9942  2997CF70
   VPICPARM.SYS  VPICPARM.SY_   15    07/24/2000  23:33      736  A3AC54B7
   VTIMER.SYS    VTIMER.SY_     16    07/24/2000  23:34    10576  D7DD634F
   WYSE.PSD      WYSE.PS_       16    07/24/2000  19:19     3072  AF5DC006

   ************************************************************************
   Product location on CSD:  A:\FIX\MPM.4
   Product name:  "IBM Multimedia Presentation Manager/2"
   Standard Edition  3.01
   Fixpak name:   XR_W043_   (Country = Generic)
   Pre-requisite CSD Level:  XR_3005_
   System Id:  1000
   Component Id:  562274700
   Archive is ON for this product.
   ________________________________________________________________________
   Product name:  "IBM Multimedia Presentation Manager/2"
   Standard Edition  1.01.2
   Fixpak name:   XR_W043_   (Country = Generic)
   Pre-requisite CSD Level:  XR_6200_
   System Id:  B020
   Component Id:  562137400
   Archive is ON for this product.
   ________________________________________________________________________

   
                       FixPak Corrective Service levels and disk layouts  55


                   October 18, 2000 - Warp 3 FixPak XR_W043

   Product name:  "IBM Multimedia Presentation Manager/2"
   Standard Edition  3.02
   Fixpak name:   XR_W043_   (Country = Generic)
   Pre-requisite CSD Level:  XR_3006_
   System Id:  1000
   Component Id:  5639A5500
   Archive is ON for this product.
   ________________________________________________________________________

   Default directories:

           ..\*

   Files contained in Fixpak for product:

   Filename      Name on CSD   Disk#  Date        Time   Size     Checksum
   ------------  ------------  -----  ----------  -----  -------  --------
   AMPMXMCD.DLL  AMPMXMCD.DL_   17    12/07/1998  09:43      544  B642596D
   AUDIOIF.DLL   AUDIOIF.DL_    17    12/07/1998  09:53      544  78F89813
   AUDIOMCD.DLL  AUDIOMCD.DL_   17    12/07/1998  09:51      544  3C92541E
   AUDIOSH.DLL   AUDIOSH.DL_    17    12/07/1998  09:38      532  F7D87B94
   AUTOPROC.DLL  AUTOPROC.DL_   17    12/07/1998  10:08    17936  DF47B61C
   AVIO.DLL      AVIO.DL_       17    12/07/1998  09:41      532  20C4245A
   CARDINFO.DLL  CARDINFO.DL_   17    12/07/1998  10:01    10768  C42FF25C
   CS4231.SYS    CS4231.SY_     17    10/08/1996  00:36    35319  ACF3AC36
   DIVE.DLL      DIVE.DL_       16    12/07/1998  09:26    69840  933863D6
   IOPRNLS.DLL   IOPRNLS.DL_    17    12/07/1998  09:25     3088  CEA8662B
   MDM.DLL       MDM.DL_        17    12/07/1998  09:28    26036  51D2A6A7
   MEMSH.DLL     MEMSH.DL_      17    12/07/1998  09:32    14144  055A0ED3
   MMPM.DLL      MMPM.DL_       17    12/07/1998  10:11   723448  CF6A2C1A
   MPGDC.DLL     MPGDC.DL_      17    12/07/1998  09:36     8912  62C9F5B5
   MPGDCS.DLL    MPGDCS.DL_     17    12/07/1998  09:36     8768  7BCEC092
   MPGIO.DLL     MPGIO.DL_      16    12/07/1998  09:37    59327  47A7FE5D
   MPGIOS.DLL    MPGIOS.DL_     16    12/07/1998  09:37    63067  508AAB7A
   MPGIOS.SCR    MPGIOS.SC_     17    10/08/1996  01:14     1053  A395762D
   R0STUB.SYS    R0STUB.SY_     17    12/07/1998  09:38     8398  C4F35C7F
   R565LUT8.LUT  R565LUT8.LU_   17    07/11/1996  18:10   263168  22446327
   SMVSMRI.DLL   SMVSMRI.DL_    17    12/07/1998  10:07     5648  0C6F8457
   SMVSPAGE.DLL  SMVSPAGE.DL_   16    12/07/1998  10:06    81440  7F50367E
   SSM.DLL       SSM.DL_        17    12/07/1998  09:25     1044  C69C1347
   SSMDD.SYS     SSMDD.SY_      17    12/07/1998  09:25    33484  5BBD8079
   SSMPEG.DLL    SSMPEG.DL_     17    12/07/1998  09:36    30160  793A067F
   SSMRES.DLL    SSMRES.DL_     17    12/07/1998  09:25    22364  F280FCD5
   SVMC.DLL      SVMC.DL_       17    12/07/1998  09:40      532  130150BF
   SVSH.DLL      SVSH.DL_       17    12/07/1998  09:42    23044  9B2235A4
   SWVR.EXE      SWVR.EX_       16    12/07/1998  10:09   152326  89AACD23
   VIDVCI.DLL    VIDVCI.DL_     16    10/19/1998  10:46    34864  41C8C682
   WAVEPROC.DLL  WAVEPROC.DL_   16    12/07/1998  10:06      532  3FA082C0
   Y644LUT8.LUT  Y644LUT8.LU_   17    07/11/1996  18:10    66560  88251A02
   YUV_LUT8.LUT  YUV_LUT8.LU_   17    07/11/1996  18:10   263168  8D29B8C1


   
                       FixPak Corrective Service levels and disk layouts  56


                   October 18, 2000 - Warp 3 FixPak XR_W043

   ************************************************************************
   Product location on CSD:  A:\FIX\OS2.5
   Product name:  "IBM OS/2 Base Operating System"
   Standard Edition  3.01
   Fixpak name:   XR_W043_   (Country = Generic)
   Pre-requisite CSD Level:  XR_3005_
   System Id:  1000
   Component Id:  562274700
   Archive is ON for this product.
   ________________________________________________________________________

   Default directories:

           ..\..\
           ..\*
           ..\..\LANGUAGE\*

   Files contained in Fixpak for product:

   Filename      Name on CSD   Disk#  Date        Time   Size     Checksum
   ------------  ------------  -----  ----------  -----  -------  --------
   FFST.DLL      FFST.DL_       18    09/05/1997  11:31    23583  8CDD7AE4
   IBMDAPIN.EXE  IBMDAPIN.EX_   18    10/25/1996  12:49    66248  34C8A147
   IBMDAPPM.EXE  IBMDAPPM.EX_   18    10/25/1996  12:49    51190  86BEC82A
   INST_DOS.EXE  INST_DOS.EX_   18    07/24/2000  21:35    36506  C87AD5F2
   LIBAUX.DLL    LIBAUX.DL_     18    09/05/1997  11:30   113848  B55CBE3C
   LIBTK.DLL     LIBTK.DL_      18    09/05/1997  11:30  1101576  BDE3379B
   NAMEADD.EXE   NAMEADD.EX_    18    07/24/2000  19:11    20045  E3D22290
   NAMECOPY.EXE  NAMECOPY.EX_   18    07/24/2000  19:11    20045  D93652E1
   NAMECSSP.DLL  NAMECSSP.DL_   18    01/21/1998  16:36    61155  ED25B521
   NAMEDEL.EXE   NAMEDEL.EX_    18    07/24/2000  19:11    20045  33567B12
   NAMEDSP.DLL   NAMEDSP.DL_    17    07/24/2000  19:08   123411  AD39D529
   NAMEDUMP.EXE  NAMEDUMP.EX_   18    07/24/2000  19:11    20045  C1652756
   NAMEEXT.EXE   NAMEEXT.EX_    18    07/24/2000  19:11    20045  F1CE1668
   NAMEFT.DLL    NAMEFT.DL_     18    01/21/1998  16:49    66306  05DC15F6
   NAMEFW.DLL    NAMEFW.DL_     18    07/24/2000  19:08    72312  C6BE3ECE
   NAMEINFO.DLL  NAMEINFO.DL_   18    07/24/2000  19:11    47925  D5284CD2
   NAMEINI.DLL   NAMEINI.DL_    18    07/24/2000  19:11    59011  B9CB85BE
   NAMEMOD.EXE   NAMEMOD.EX_    18    07/24/2000  19:11    20045  DF495A55
   NAMEMOVE.EXE  NAMEMOVE.EX_   17    07/24/2000  19:11    20045  3F809E14
   NAMEOSP.DLL   NAMEOSP.DL_    18    07/24/2000  19:10    52709  6737BF8B
   NAMEREXX.DLL  NAMEREXX.DL_   17    07/24/2000  19:11   156291  DD122EFA
   NAMEREXX.MSG  NAMEREXX.MS_   18    01/21/1998  16:47     4257  D09A395D
   OS2NS.EXE     OS2NS.EX_      18    07/24/2000  19:10    44964  167DBD57
   PMDDEML.DLL   PMDDEML.DL_    18    07/24/2000  20:40    27210  2E45543A
   PMWINX.DLL    PMWINX.DL_     17    07/24/2000  21:35   520559  AE7B8ED7
   RSRV.EXE      RSRV.EX_       18    07/24/2000  19:08    77955  6EF40617





   
                       FixPak Corrective Service levels and disk layouts  57


                   October 18, 2000 - Warp 3 FixPak XR_W043

   12.0 SPACE UTILIZATION

   The FixPak installation process requires free space on the following
   drives:

   Space needed   Drive

   Up to 2MB      C:

   Up to 2MB      Boot drive (4MB if boot is C:)

   Up to 22MB     Drive with most free space, holds deferred files if
                  A:SERVICE method used.

   Up to 32MB     FixPak Archive/Backup for product with CSD level of
                  XR_3005

   Up to 33MB     FixPak Archive/Backup for product with CSD level of
                  XR_3006

   Up to 3MB      FixPak Archive/Backup for product with CSD level of
                  XR_6200

   Note: The lines labeled "FixPak Archive/Backup for product with CSD level
   of" will be on the drive you specify and will occupy up to the size
   indicated for the Archive and for the Backup directories. If, for
   example, the indicated size is 30MB then the space actually occupied on
   the drive can be up to 60MB.
























   
                                                       Space Utilization  58


                   October 18, 2000 - Warp 3 FixPak XR_W043

   13.0 RECOVERING FIXPAK ARCHIVE AND BACKUP SPACE

   Warning: Make sure you read and understand the following before removing
   the Archive and Backup files and directories.

   You can recover the space used for FixPak Archive and Backup files as
   long as you understand that doing this prevents you from being able to
   backout to the previous Backup or Archive level. If it becomes necessary
   at a later time to backout a FixPak, the only way you can do this is to
   reinstall Warp.

   Do the following to delete the FixPak Backup and Archive files and remove
   the files used by CSF to keep track of what service has been applied to
   your system.

   1.  Delete every instance of the following files on your system
       (search every drive and every directory they contain).
       Ž   LOGF0000.*   (can be OS2 or MPM)
       Ž   LOGSTART.*   (can be OS2 or MPM)
       Ž   LOGARCH.*    (can be OS2 or MPM)
       Ž   CSF_*.*
       Ž   FIXSTART
   2.  Delete the files in the FixPak Archive and Backup directories on
       your harddisk.
   3.  Remove the FixPak Archive and Backup directories with the RMDIR
       command.


























   
                              Recovering FixPak ARCHIVE and BACKUP space  59


                   October 18, 2000 - Warp 3 FixPak XR_W043

   14.0 RECOVERING FROM PROBLEMS

   See the file "README.TIP" for information on recovering from FixPak
   installation problems and resolving problems after the FixPak is
   installed.  It is located on the first FixPak disk which is:

   FixPak XR_W043 Corrective Service Diskette 1 (CSF DISK 1).


   This file is setup to print at 60 lines per page.










































   
                                                Recovering from problems  60
